For 1990-2009 cars

### Removal Procedure

Note: To remove the power steering pump belt, do remove the accessory belt in advance.

1. Rotate the tensioner star-nut (1) and remove the accessory belt.
2. Remove the power steering belt. Refer to Refer to Power Steering Pump Replacement.

### Installation Procedure

1. Install the power steering belt. Refer to Power Steering Pump Replacement.
2. Rotate the tensioner star-nut (1) and install the accessory belt.
3. Install the engine front shield at the position of right front wheel.