For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the engine cover bolts and the nuts.
3. Remove the engine cover.
4. Disconnect the camshaft position (CMP) sensor electrical connector.
5. Remove the timing belt front cover. Refer to Timing Belt Replacement .

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the CMP sensor and bolt.

Tighten
Tighten the CMP sensor bolts to 7 N·m (62 lb in).

2. Install the timing bolt front cover. Refer to Timing Belt Replacement .
3. Connect the CMP sensor electrical connector.
4. Install the engine cover.
5. Connect the negative battery cable.