For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Locate the vessel for containing engine oil beneath drain plug of the vehicle.
3. Remove the oil drain (2) carefully.
4. Drain the engine oil.
5. Remove the oil filter cap (1).
6. Remove the oil filter.

### Installation Procedure

Note: Do not re-use the engine oil filter.

1. Install the new oil filter.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the oil filter cap (1) and tighten to 25 N·m (18.4 lb ft).

Note: Refer to engine oil specifications in the owners manual and refill with the recommended engine oil and quantity.

3. Install the drain plug (2) and tighten to 9 N·m (79.7 lb in).
4. Open the oil filling cap.
5. Refill the new engine oil.