For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel lower cover.
3. Reach underneath the instrument panel and remove the bolts and the daytime running lamp module.
4. Disconnect the electrical connector.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the daytime running lamp module with the bolts and tighten to 2.5 N·m (22 lb in).
2. Connect the electrical connector.
3. Install the instrument panel lower cover.
4. Connect the negative battery cable.