For 1990-2009 cars

### Removal Procedure

1. Loosen the air cleaner intake duct clamp at the air cleaner assembly.
2. Remove the air cleaner intake duct from the upper air cleaner cover.
3. Remove the upper air cleaner screws.
4. Remove the upper air cleaner cover from the lower air cleaner housing.
5. Remove the air cleaner filter from lower air cleaner housing.

### Installation Procedure

1. Install the air cleaner filter into the lower air cleaner housing.
2. Install the upper air cleaner cover to lower air cleaner housing.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the upper air cleaner screws.

Tighten
Tighten the upper air cleaner cover screws to 3 N·m (27 lb in).

4. Install the intake duct to the upper air cleaner cover.

Tighten
Tighten the intake duct clamp to 3 N·m (27 lb in).