For 1990-2009 cars

Table 1: | Too Much Play in Steering System
Table 2: | Rattle in Rack and Pinion Steering Gear

#### Too Much Play in Steering System

Checks | Actions
--- | ---
Check the steering gear adjustment. | Perform the straight-ahead check.
Check the wheel bearing for wear or damage. | Replace the wheel bearing.
Check the outer tie rods for improper installation. | Tighten the tie rods.

#### Rattle in Rack and Pinion Steering Gear

Checks | Actions
--- | ---
Check the steering gear for improper and insufficient lubrication. | Lubricate the rack assembly. Lubricate the pinion assembly.
Check the steering gear mounting for improper installation. | Tighten the steering gear mounting bolts and the nuts.
Check the outer tie rods for improper installation. | Tighten the tie rods.