For 1990-2009 cars

### Removal Procedure

Caution: Refer to Sensing and Diagnostic Module Voltage after Ignition is Turned Off Caution in the Preface section.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the connector (1) from the front air bag sensor (3).
3. Remove the front air bag sensor mounting bolt (2).
4. Remove the front air bag sensor.

### Installation Procedure

1. Install the front air bag sensor.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front air bag sensor mounting bolt (2).

Tighten
Tighten the side air bag sensor mounting bolts to 10 N·m (89 lb in).

3. Connect the connector (1) to the front air bag sensor (3).
4. Connect the negative battery cable.