For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the breather hose from the valve cover.
3. Remove the 8 bolts from the valve cover.
4. Remove the valve cover.
5. Remove the valve cover gasket.
6. Clean the sealing surfaces of the valve cover and the camshaft housing.

### Installation Procedure

1. Install the new valve cover gasket and the valve cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the 8 bolts to the valve cover.

Tighten
Tighten the valve cover bolts to 9 N·m (80 lb in).

3. Connect the breather tube to the valve cover.
4. Connect the negative battery cable.