For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

Caution: Refer to Fuel Pressure Caution in the Preface section.

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the EVAP canister purge valve upper and lower hoses.
3. Disconnect the EVAP canister purge valve connector.
4. Detach the EVAP canister purge valve (1).

### Installation Procedure

1. Install the EVAP canister purge valve (1).
2. Connect the EVAP canister purge valve connector.
3. Connect the EVAP canister purge valve upper and lower hoses.
4. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.