For 1990-2009 cars

## Door Window Regulator Replacement Manual Front

### Removal Procedure

1. Remove the front door glass. Refer to Front Side Door Window Replacement.
2. Remove the nuts and the window regulator.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the window regulator and the nuts and tighten to 7 N·m (62 lb in).
2. Install the front door glass. Refer to Front Side Door Window Replacement.

## Door Window Regulator Replacement Manual Rear

### Removal Procedure

1. Remove the rear door glass. Refer to Rear Side Door Window Replacement.
2. Remove the nuts and the window regulator.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the window regulator with the nuts and tighten to 7 N·m (62 lb in).
2. Install the rear door glass. Refer to Rear Side Door Window Replacement.

## Door Window Regulator Replacement Power Front

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the door glass. Refer to Front Side Door Window Replacement.
3. Remove the nuts and the regulator.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the window regulator with the nuts and tighten to 7 N·m (62 lb in).
3. Install the front door glass. Refer to Front Side Door Window Replacement.
4. Connect the negative battery cable.
5. If the vehicle is equipped with a one touch up function, and the driver side power window regulator has been replaced, perform the window motor reinitialization process. Refer to Power Window Reinitialization.

## Door Window Regulator Replacement Power Rear

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear door glass. Refer to Rear Side Door Window Replacement.
3. Remove the nuts and the regulator.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the window regulator with the nuts and tighten to 7 N·m (62 lb in).
3. Install the rear door glass. Refer to Rear Side Door Window Replacement.
4. Connect the negative battery cable.