For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.

Notice: Refer to Vehicle Lifting and Jacking Notice in the Preface section.

2. Raise and suitably support the vehicle.
3. Disconnect the electrical connector for the rear wheel speed sensor from the rear axle.
4. Remove the mounting bolt from the rear wheel speed sensor.
5. Remove the cable grommets from the rear wheel speed sensor, and remove the speed sensor.

### Installation Procedure

1. Install the rear wheel speed sensor, and install the cable grommets.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear wheel sensor mounting bolt.

Tighten
Tighten the bolt to 9 N·m (80 lb in).

3. Connect the electrical connector for the rear wheel speed sensor to the rear axle.
4. Lower the vehicle.
5. Connect the negative battery cable.