For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat back lock release knob.
2. Reposition the rear seat back cover.
3. Remove the screws and the lock assembly.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear seat back lock assembly with the screws and tighten to 20 N·m (15 lb ft).
2. Install the rear seat back cover to its original position.
3. Install the rear seat back lock release knob.