For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear side marker lamp assembly.
3. Remove the bulb from the rear side marker lamp assembly.

### Installation Procedure

1. Install the bulb into the side marker lamp assembly.
2. Install the side marker lamp into the bumper fascia.
3. Connect the negative battery cable.