For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
2. Lift the vehicle up.
3. Remove the front-right tire and wheel.
4. Remove the engine under cover.
5. Remove the power steering pump bracket retaining bolts and loosen the belt.
6. Remove the power steering pump-air compressor belt.
7. Rotate the inner hex of the tensioner nut counterclockwise and loosen the nut.
8. Rotate the outer hex of the tensioner nut clockwise and put down the tensioner.
9. Remove the water pump-generator belt.
10. Remove the generator. Refer to Generator Replacement
11. Remove the accessory tensioner (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the accessory tensioner (2).

Tighten
Tighten the accessory tensioner retaining bolts (1) to 33 N·m (24.3 lb ft).

2. Install the generator. Refer to Generator Replacement.
3. Rotate the outer hex of the tensioner nut counterclockwise and put up the tensioner.
4. Rotate the inner hex of the tensioner nut clockwise and tighten the nut, installing the water pump-generator belt.
5. Install the power steering pump-air compressor belt (1), tightening power steering pump bracket retaining bolts.

Tighten
Tighten the power steering pump bracket mounting bolts to 20 N·m (14.7 lb ft).

6. Install the engine undercover.
7. Lower the vehicle.
8. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.