For 1990-2009 cars

### Cruise Control Clutch Switch Adjustment

1. Push the switch assembly through the pedal support and turn 90 degrees.
2. Hold the clutch pedal to the rest position.
3. Connect the cruise control clutch pedal switch electrical connector.
4. Verify the operation of the clutch switch by operating the cruise control and checking the clutch switch stops operation of the cruise control when the clutch pedal is pressed.