For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster trim panel.
3. Remove the screws and the instrument cluster.
4. Disconnect the electrical connectors.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Connect the electrical connectors.
2. Install the instrument cluster with the screws.
3. Install the instrument cluster trim panel.
4. Connect the negative battery cable.