For 1990-2009 cars

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
B0996 | Vehicle Electronic Control Unit (ECU) VIN Check Error | TDM | DTC B0996
B1000 | Electronic Control Unit (ECU) Performance | TDM | DTC B1000
B1015 | Vehicle Identification Number (VIN) Information Error | TDM | DTC B1015
B1016 | Vehicle Identification Number (VIN) Information Not Programmed | TDM | DTC B1016
B1101 | Battery Voltage High | SDM | DTC B1101
B1102 | Battery Voltage Low | SDM | DTC B1102
B1103 | SIR Serial Communications Fault | SDM | DTC B1103
B1104 | Passenger Seat Occupant Classification System (OCS) Voltage Out of Range | SDM | DTC B1104
B1326 | Front End Sensor 1 Short to Ground | SDM | DTC B1326
B1327 | Front End Sensor 1 Short to Battery | SDM | DTC B1327
B1328 | Front End Sensor 1 Internal Electronic Failure | SDM | DTC B1328
B1329 | Front End Sensor 1 Invalid Serial Data Received | SDM | DTC B1329
B1330 | Incorrect Electronic Front End Sensor 1 Installed | SDM | DTC B1330
B1331 | Front End Sensor 2 Short to Ground | SDM | DTC B1331
B1332 | Front End Sensor 2 Short to Battery | SDM | DTC B1332
B1333 | Front End Sensor 2 Internal Electronic Failure | SDM | DTC B1333
B1334 | Front End Sensor 2 Invalid Serial Data Received | SDM | DTC B1334
B1335 | Incorrect Electronic Front End Sensor 2 Installed | SDM | DTC B1335
B1346 | Driver Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1346
B1347 | Driver Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1347
B1348 | Driver Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1348
B1349 | Driver Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1349
B1352 | Passenger Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1352
B1353 | Passenger Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1353
B1354 | Passenger Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1354
B1355 | Passenger Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1355
B1361 | Driver Pretensioner Deployment Loop Resistance High | SDM | DTC B1361
B1362 | Driver Pretensioner Deployment Loop Resistance Low | SDM | DTC B1362
B1363 | Driver Pretensioner Deployment Loop Short to Ground | SDM | DTC B1363
B1364 | Driver Pretensioner Deployment Loop Short to Battery | SDM | DTC B1364
B1367 | Passenger Pretensioner Deployment Loop Resistance High | SDM | DTC B1367
B1368 | Passenger Pretensioner Deployment Loop Resistance Low | SDM | DTC B1368
B1369 | Passenger Pretensioner Deployment Loop Short to Ground | SDM | DTC B1369
B1370 | Passenger Pretensioner Deployment Loop Short to Battery | SDM | DTC B1370
B1378 | LF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1378
B1379 | LF Side Deployment Loop Resistance Low | SDM | DTC B1379
B1380 | LF Side Deployment Loop Short to Ground | SDM | DTC B1380
B1381 | LF Side Deployment Loop Short to Battery | SDM | DTC B1381
B1382 | RF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1382
B1383 | RF Side Deployment Loop Resistance Low | SDM | DTC B1383
B1384 | RF Side Deployment Loop Short to Ground | SDM | DTC B1384
B1385 | RF Side Deployment Loop Short to Battery | SDM | DTC B1385
B1395 | Deployment Loops Interconnect Circuit | SDM | DTC B1395
B1400 | Driver SIS Malfunction | SDM | DTC B1400
B1401 | LF Side Impact Sensor Short to Ground | SDM | DTC B1401
B1402 | LF Side Impact Sensor Short to Battery | SDM | DTC B1402
B1403 | Passenger SIS Malfunction | SDM | DTC B1403
B1404 | RF Side Impact Sensor Short to Ground | SDM | DTC B1404
B1405 | RF Side Impact Sensor Short to Battery | SDM | DTC B1405
B1409 | LF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1409
B1410 | RF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1410
B1414 | LF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1414
B1415 | RF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1415
B1424 | Device 1 Voltage Low | TDM | DTC B1424
B1440 | Passenger Seat Occupant Classification System (OCS) Short to Ground | SDM | DTC B1440
B1446 | Passenger Seat Occupant Classification System (OCS) Short to Battery | SDM | DTC B1446
B1447 | Passenger Seat Occupant Classification System (OCS) Sensor Circuit | SDM | DTC B1447
B1448 | Passenger Seat Occupant Classification System (OCS) Sensor | SDM | DTC B1448
B1449 | Passenger Seat Occupant Classification Sensor Communication | SDM | DTC B1449
B1450 | Incorrect Passenger Seat Occupant Classification Sensor Installed | SDM | DTC B1450
B1481 | Driver Frontal Deployment Loop Stage 2 Resistance Above Threshold | SDM | DTC B1481
B1482 | Driver Frontal Deployment Loop Stage 2 Resistance Below Threshold | SDM | DTC B1482
B1483 | Driver Frontal Deployment Loop Stage 2 Short to Ground | SDM | DTC B1483
B1484 | Driver Frontal Deployment Loop Stage 2 Short to Battery | SDM | DTC B1484
B1485 | Passenger Frontal Deployment Loop Stage 2 Resistance Above Threshold | SDM | DTC B1485
B1486 | Passenger Frontal Deployment Loop Stage 2 Resistance Below Threshold | SDM | DTC B1486
B1487 | Passenger Frontal Deployment Loop Stage 2 Short to Ground | SDM | DTC B1487
B1488 | Passenger Frontal Deployment Loop Stage 2 Short to Battery | SDM | DTC B1488
B1620 | ECU Performance | SDM | DTC B1620
B1650 | Frontal Stage 1 Deployment Commanded | SDM | DTC B1650
B1651 | LH Side Air Bag Deployment Commanded | SDM | DTC B1651
B1652 | RH Side Air Bag Deployment Commanded | SDM | DTC B1652
B1657 | Deployment Commanded Pretensioner | SDM | DTC B1657
B1670 | Frontal Stage 2 Deployment Commanded | SDM | DTC B1670
B2500 | Inflatable Restraint System Indicator Circuit | SDM | DTC B2500
B2501 | Passenger Air Bag Disabled Indicator Circuit Malfunction | SDM | DTC B2501
B2502 | Passenger Air Bag Disabled Indicator Circuit Malfunction | SDM | DTC B2502
B302A | Telematic Requested Immobilization | TDM | DTC B302A
B3031 | Security System Controller In Learn Mode | TDM | DTC B3031
B3035 | No Transponder Modulation or No Transponder | TDM | DTC B3035
B3060 | Unprogrammed Transponder Identification Code Received | TDM | DTC B3060
B3935 | Transponder Authentication Error | TDM | DTC B3935
B3976 | Unconfigured Transponder/Vehicle Configuration Not Programmed | TDM | DTC B3976
P0010 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit | ECM | DTC P0010 or P0013
P0011 | Intake Camshaft Position (CMP) System Performance | ECM | DTC P0011, P0012, P0014, or P0015 for the 1.4 L engine (LDT) or DTC P0011 or P0014 for the 1.6 L engine (LXV)
P0013 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit | ECM | DTC P0010 or P0013
P0014 | Exhaust Camshaft Position (CMP) System Performance | ECM | DTC P0011 or P0014
P0016 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation | ECM | DTC P0016 or P0340 for the 1.6 L engine (LXT) or DTC P0016 or P0017 for the 1.6 L engine (LXV)
P0017 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation | ECM | DTC P0016 or P0017
P0030 | HO2S Heater Control Circuit Sensor 1 | ECM | DTC P0030, P0036, P0053, P0054, P0135, or P0141
P0031 | H02S Heater Control Circuit Low Voltage Sensor 1 | ECM | DTC P0031, P0032, P0037, or P0038 for the 1.2 L engine or DTC P0031, P0032, P0037, or P0038 for the 1.6 L engine (LXT)
P0032 | H02S Heater Control Circuit High Voltage Sensor 1 | ECM | DTC P0031, P0032, P0037, or P0038 for the 1.2 L engine or DTC P0031, P0032, P0037, or P0038 for the 1.6 L engine (LXT)
P0036 | HO2S Heater Control Circuit Sensor 2 | ECM | DTC P0030, P0036, P0053, P0054, P0135, or P0141
P0037 | H02S Heater Control Circuit Low Voltage Sensor 2 | ECM | DTC P0031, P0032, P0037, or P0038 for the 1.2 L engine or DTC P0031, P0032, P0037, or P0038 for the 1.6 L engine (LXT)
P0038 | H02S Heater Control Circuit High Voltage Sensor 2 | ECM | DTC P0031, P0032, P0037, or P0038 for the 1.2 L engine or DTC P0031, P0032, P0037, or P0038 for the 1.6 L engine (LXT)
P0053 | HO2S Heater Resistance Circuit Sensor 1 | ECM | DTC P0030, P0036, P0053, P0054, P0135, or P0141
P0054 | HO2S Heater Resistance Circuit Sensor 2 | ECM | DTC P0030, P0036, P0053, P0054, P0135, or P0141
P0068 | Throttle Body Airflow Performance | ECM | DTC P0068 for the 1.6 L engine (LXT) or DTC P0068 or P1101 for the 1.6 L (LXV)
P0101 | Mass Air Flow (MAF) Sensor Performance | ECM | DTC P0101
P0102 | Mass Air Flow (MAF) Sensor Circuit Low Frequency | ECM | DTC P0102 or P0103
P0103 | Mass Air Flow (MAF) Sensor Circuit High Frequency | ECM | DTC P0102 or P0103
P0106 | Manifold Absolute Pressure (MAP) Sensor Performance | ECM |

• | DTC P0106 for the 1.4 L engine (L95)

• | DTC P0106 for the 1.6 L engine (LXT)

• | DTC P0106 for the 1.6 L engine (LXV)

P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | ECM |

• | DTC P0107 or P0108 for the 1.2 L engine

• | DTC P0107 or P0108 for the 1.4 L engine (L95)

• | DTC P0107 or P0108 for the 1.5 L engine

• | DTC P0107 or P0108 for the 1.6 L engine (LXT)

• | DTC P0107 or P0108 for the 1.6 L engine (LXV)

P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | ECM |

• | DTC P0107 or P0108 for the 1.2 L engine

• | DTC P0107 or P0108 for the 1.4 L engine (L95)

• | DTC P0107 or P0108 for the 1.5 L engine

• | DTC P0107 or P0108 for the 1.6 L engine (LXT)

• | DTC P0107 or P0108 for the 1.6 L engine (LXV)

P0110 | Intake Air Temperature (IAT) Sensor Circuit | ECM | DTC P0110 or P0111
P0111 | Intake Air Temperature (IAT) Sensor Performance | ECM | DTC P0110 or P0111
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM |

• | DTC P0112 or P0113 for the 1.2 L engine

• | DTC P0112 or P0113 for the 1.4 L engine (L95)

• | DTC P0112 or P0113 for the 1.5 L engine

• | DTC P0112 or P0113 for the 1.6 L engine (LXT)

• | DTC P0112 or P0113 for the 1.6 L engine (LXV)

P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM |

• | DTC P0112 or P0113 for the 1.2 L engine

• | DTC P0112 or P0113 for the 1.4 L engine (L95)

• | DTC P0112 or P0113 for the 1.5 L engine

• | DTC P0112 or P0113 for the 1.6 L engine (LXT)

• | DTC P0112 or P0113 for the 1.6 L engine (LXV)

P0114 | Intake Air Temperature (IAT) Sensor Circuit Intermittent | ECM | DTC P0114
P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P0116 for the 1.6 L engine (LXT) or DTC P0116 for the 1.6 L engine (LXV)
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM |

• | DTC P0117 or P0118 for the 1.2 L engine

• | DTC P0117 or P0118 for the 1.4 L engine (L95)

• | DTC P0117 or P0118 for the 1.5 L engine

• | DTC P0117 or P0118 for the 1.6 L engine (LXT)

• | DTC P0117 or P0118 for the 1.6 L engine (LXV)

P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM |

• | DTC P0117 or P0118 for the 1.2 L engine

• | DTC P0117 or P0118 for the 1.4 L engine (L95)

• | DTC P0117 or P0118 for the 1.5 L engine

• | DTC P0117 or P0118 for the 1.6 L engine (LXT)

• | DTC P0117 or P0118 for the 1.6 L engine (LXV)

P0122 | Throttle Position (TP) Sensor Circuit Low Voltage | ECM |

• | DTC P0122 or P0123 for the 1.2 L engine

• | DTC P0122 or P0123 for the 1.4 L engine (L95)

• | DTC P0122 or P0123 for the 1.5 L engine

• | DTC P0122, P0123, P0222, P0223, or P2135 for the 1.6 L engine (LXT)

• | DTC P0121-P0123, P0222, P0223, or P2135 for the 1.6 L engine (LXV)

P0123 | Throttle Position (TP) Sensor Circuit High Voltage | ECM |

• | DTC P0122 or P0123 for the 1.2 L engine

• | DTC P0122 or P0123 for the 1.4 L engine (L95)

• | DTC P0122 or P0123 for the 1.5 L engine

• | DTC P0122, P0123, P0222, P0223, or P2135 for the 1.6 L engine (LXT)

• | DTC P0121-P0123, P0222, P0223, or P2135 for the 1.6 L engine (LXV)

P0125 | Engine Coolant Temperature (ECT) Insufficient for Close Loop | ECM | DTC P0125 or P0128
P0126 | Engine Coolant Temperature (ECT) Insufficient for Closed Loop | ECM | DTC P0126
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM | DTC P0125 or P0128 for the 1.6 L engine (LXT) or DTC P0128 for the 1.6 L engine (LXV)
P0131 | HO2S Circuit Low Voltage Sensor 1 | ECM |

• | DTC P0131 or P0137 for the 1.2 L engine

• | DTC P0131 or P0132 for the 1.4 L engine (L95)

• | DTC P0131 or P0132 for the 1.5 L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6 L engine (LXT)

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6 L engine (LXV)

P0132 | HO2S Circuit High Voltage Sensor 1 | ECM |

• | DTC P0132 or P0138 for the 1.2 L engine

• | DTC P0131 or P0132 for the 1.4 L engine (L95)

• | DTC P0131 or P0132 for the 1.5 L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6 L engine (LXV)

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6 L engine (LXT)

P0133 | HO2S Slow Response Sensor 1 | ECM |

• | DTC P0133 or P0139 for the 1.2 L engine

• | DTC P0133, P1133, or P1134 for the 1.4 L engine (L95)

• | DTC P0133 or P0139 for the 1.6 L engine (LXT)

• | DTC P0133 or P1133 for the 1.6 L engine (LXV)

P0134 | HO2S Circuit Insufficient Activity Sensor 1 | ECM |

• | DTC P0134 or P0140 for the 1.2 L engine

• | DTC P0134 or P0140 for the 1.4 L engine (L95)

• | DTC P0134 for the 1.5 L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6 L engine (LXT)

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6 L engine (LXV)

P0135 | HO2S Heater Performance Sensor 1 | ECM |

• | DTC P0135 or P0141 for the 1.4L (L95) engine

• | DTC P0135 or P0141 for the 1.6 L engine (LXT)

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 1.6 L engine (LXV)

P0137 | HO2S Circuit Low Voltage Sensor 2 | ECM |

• | DTC P0131 or P0137 for the 1.2 L engine

• | DTC P0137 or P0138 for the 1.4 L engine (L95)

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6 L engine (LXT)

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6 L engine (LXV)

P0138 | HO2S Circuit High Voltage Sensor 2 | ECM |

• | DTC P0132 or P0138 for the 1.2 L engine

• | DTC P0137 or P0138 for the 1.4 L engine (L95)

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6 L engine (LXT)

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6 L engine (LXV)

P0139 | HO2S Slow Response Sensor 2 | ECM | DTC P0133 or P0139 for the 1.2 L engine or DTC P0133 or P0139 for the 1.6 L engine (LXT)
P0140 | HO2S Circuit Insufficient Activity Sensor 2 | ECM |

• | DTC P0134 or P0140 for the 1.2 L engine

• | DTC P0134 or P0140 for the 1.4 L engine (L95)

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6 L engine (LXT)

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6 L engine (LXV)

P0141 | H02S Heater Performance Sensor 2 | ECM |

• | DTC P0135 or P0141 for the 1.4L (L95) engine

• | DTC P0135 or P0141 for the 1.6 L engine (LXT)

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 1.6 L engine (LXV)

P0171 | Fuel Trim System Lean | ECM |

• | DTC P0171 or P0172 for the 1.2 L engine

• | DTC P0171 or P0172 for the 1.4 L engine (L95)

• | DTC P0171, P0172, P2187, or P2188 for the 1.6 L engine (LXT)

• | DTC P0171 or P0172 for the 1.6 L engine (LXV)

P0172 | Fuel Trim System Rich | ECM |

• | DTC P0171 or P0172 for the 1.2 L engine

• | DTC P0171 or P0172 for the 1.4 L engine (L95)

• | DTC P0171, P0172, P2187, or P2188 for the 1.6 L engine (LXT)

• | DTC P0171 or P0172 for the 1.6 L engine (LXV)

P0201 | Injector 1 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4 L engine (L95)

• | DTC P0201, P0202, P0203, or P0204 for the 1.5 L engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.6 L engine (LXT)

• | DTC P0201, P0202, P0203, or P0204 for the 1.6 L engine (LXV)

P0202 | Injector 2 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4 L engine (L95)

• | DTC P0201, P0202, P0203, or P0204 for the 1.5 L engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.6 L engine (LXT)

• | DTC P0201, P0202, P0203, or P0204 for the 1.6 L engine (LXV)

P0203 | Injector 3 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4 L engine (L95)

• | DTC P0201, P0202, P0203, or P0204 for the 1.5 L engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.6 L engine (LXT)

• | DTC P0201, P0202, P0203, or P0204 for the 1.6 L engine (LXV)

P0204 | Injector 4 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4 L engine (L95)

• | DTC P0201, P0202, P0203, or P0204 for the 1.5 L engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.6 L engine (LXT)

• | DTC P0201, P0202, P0203, or P0204 for the 1.6 L engine (LXV)

P0217 | Engine Coolant Over Temperature | ECM | DTC P0217
P0222 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, P0223, or P2135 for the 1.6 L engine (LXT) or DTC P0121-P0123, P0222, P0223, or P2135 for the 1.6 L engine (LXV)
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0122, P0123, P0222, P0223, or P2135 for the 1.6 L engine (LXT) or DTC P0121-P0123, P0222, P0223, or P2135 for the 1.6 L engine (LXV)
P0230 | Fuel Pump Relay Control Circuit | ECM | DTC P0230
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2 L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6 L engine (LXT)
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2 L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6 L engine (LXT)
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2 L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6 L engine (LXT)
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2 L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6 L engine (LXT)
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2 L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6 L engine (LXT)
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2 L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6 L engine (LXT)
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2 L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6 L engine (LXT)
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2 L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6 L engine (LXT)
P0300 | Engine Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.2 L engine

• | DTC P0300-P0304 for the 1.4 L engine (L95)

• | DTC P0300-P0304 for the 1.6 L engine (LXT)

• | DTC P0300-P0304 for the 1.6 L engine (LXV)

P0301 | Cylinder 1 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4 L engine (L95)

• | DTC P0300-P0304 for the 1.6 L engine (LXT)

• | DTC P0300-P0304 for the 1.6 L engine (LXV)

P0302 | Cylinder 2 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4 L engine (L95)

• | DTC P0300-P0304 for the 1.6 L engine (LXT)

• | DTC P0300-P0304 for the 1.6 L engine (LXV)

P0303 | Cylinder 3 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4 L engine (L95)

• | DTC P0300-P0304 for the 1.6 L engine (LXT)

• | DTC P0300-P0304 for the 1.6 L engine (LXV)

P0304 | Cylinder 4 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4 L engine (L95)

• | DTC P0300-P0304 for the 1.6 L engine (LXT)

• | DTC P0300-P0304 for the 1.6 L engine (LXV)

P0313 | Misfire Detected With Low Fuel Level | ECM | DTC P0313
P0314 | Single Cylinder Engine Misfire Detected | ECM | DTC P0314
P0315 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P0315 for the 1.6 L engine (LXT) or DTC P0315 for the 1.6 L engine (LXV)
P0317 | Rough Road Signal Not Detected | ECM | DTC P0317 for the 1.4 L engine (L95) or DTC P0317 for the 1.6 L engine (LXT)
P0324 | Knock Sensor (KS) Module Performance | ECM |

• | DTC P0324 for the 1.4 L engine (L95)

• | DTC P0324 for the 1.6 L engine (LXT)

• | DTC P0324, P0326, or P06B6 for the 1.6 L engine (LXV)

P0325 | Knock Sensor (KS) Module Performance Non European Emissions Knock Sensor (KS) Circuit European Emissions | ECM |

• | DTC P0325 for the 1.4 L engine (L95)

• | DTC P0325 for the 1.5L engine

• | DTC P0325 for the 1.6 L engine (LXT)

P0326 | Knock Sensor (KS) Performance | ECM | DTC P0324, P0326, or P06B6
P0327 | Knock Sensor (KS) Circuit | ECM |

• | DTC P0327 for the 1.2 L engine

• | DTC P0327 for the 1.4 L engine (L95)

• | DTC P0327 for the 1.5 L engine

P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM |

• | DTC P0335, P0336, or P0337 for the 1.2 L engine

• | DTC P0335 or P0336 for the 1.6 L engine (LXT)

• | DTC P0335 or P0336 for the 1.6 L engine (LXV)

P0336 | Crankshaft Position (CKP) Sensor Performance | ECM |

• | DTC P0335, P0336, or P0337 for the 1.2 L engine

• | DTC P0335, P0336, or P0337 for the 1.4 L engine (L95)

• | DTC P0336 or P0337 for the 1.5 L engine

• | DTC P0335 or P0336 for the 1.6 L engine (LXT)

• | DTC P0335 or P0336 for the 1.6 L engine (LXV)

P0337 | Crankshaft Position (CKP) Sensor Circuit Low Duty Cycle | ECM |

• | DTC P0335, P0336, or P0337 for the 1.2 L engine

• | DTC P0335, P0336, or P0337 for the 1.4 L engine (L95)

• | DTC P0336 or P0337 for the 1.5 L engine

P0340 | Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0016 or P0340 for the 1.6 L engine (LXT) or DTC P0340 or P0365 for the 1.6 L engine (LXV)
P0341 | Camshaft Position (CMP) Sensor Performance | ECM |

• | DTC P0341 or P0342 for the 1.2 L engine

• | DTC P0341 or P0342 for the 1.4 L engine (L95)

• | DTC P0341 or P0342 for the 1.5 L engine

• | DTC P0341 or P0366 for the 1.6 L engine (LXV)

P0342 | Camshaft Position (CMP) Sensor Circuit Low Voltage | ECM |

• | DTC P0341 or P0342 for the 1.2 L engine

• | DTC P0341 or P0342 for the 1.4 L engine (L95)

• | DTC P0341 or P0342 for the 1.5 L engine

P0351 | Ignition Coil 1 and 4 Control Circuit | ECM |

• | DTC P0351 or P0352 for the 1.2 L engine

• | DTC P0351 or P0352 for the 1.4 L engine (L95)

• | DTC P0351 or P0352 for the 1.5 L engine

• | DTC P0351 or P0352 for the 1.6 L engine (LXT)

• | DTC P0351-P0354 for the 1.6 L engine (LXV)

P0352 | Ignition Coil 2 and 3 Control Circuit | ECM |

• | DTC P0351 or P0352 for the 1.2 L engine

• | DTC P0351 or P0352 for the 1.4 L engine (L95)

• | DTC P0351 or P0352 for the 1.5 L engine

• | DTC P0351 or P0352 for the 1.6 L engine (LXT)

• | DTC P0351-P0354 for the 1.6 L engine (LXV)

P0353 | Ignition Coil 3 Control Circuit | ECM | DTC P0351-P0354
P0354 | Ignition Coil 4 Control Circuit | ECM | DTC P0351-P0354
P0365 | Exhaust Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0340 or P0365
P0366 | Exhaust Camshaft Position (CMP) Sensor Performance | ECM | DTC P0341 or P0366
P0400 | Exhaust Gas Recirculation (EGR) Flow Incorrect | ECM |

• | DTC P0400, P0401, or P0402 for the 1.2 L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6 L engine (LXT)

P0401 | Exhaust Gas Recirculation (EGR) Flow Insufficient | ECM |

• | DTC P0400, P0401, or P0402 for the 1.2 L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4 L engine (L95)

• | DTC P0400, P0401, P0402, or P1402 for the 1.6 L engine (LXT)

P0402 | Exhaust Gas Recirculation (EGR) Flow Excessive | ECM |

• | DTC P0400, P0401, or P0402 for the 1.2 L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4 L engine (L95)

• | DTC P0400, P0401, P0402, or P1402 for the 1.6 L engine (LXT)

P0403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | ECM | DTC P0403, P0404, P0405, or P0406 for the 1.2 L engine or DTC P0403, P0404, P0405, P0406, or P042E for the 1.6 L engine (LXT)
P0404 | Exhaust Gas Recirculation (EGR) Open Position Performance | ECM |

• | DTC P0403, P0404, P0405, or P0406 for the 1.2 L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4 L engine (L95)

• | DTC P0403, P0404, P0405, P0406, or P042E for the 1.6 L engine (LXT)

P0405 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit Low Voltage | ECM |

• | DTC P0403, P0404, P0405, or P0406 for the 1.2 L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4 L engine (L95)

• | DTC P0403, P0404, P0405, P0406, or P042E for the 1.6 L engine (LXT)

P0406 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit High Voltage | ECM |

• | DTC P0403, P0404, P0405, or P0406 for the 1.2 L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4 L engine (L95)

• | DTC P0403, P0404, P0405, P0406, or P042E for the 1.6 L engine (LXT)

P0420 | Catalyst System Low Efficiency | ECM |

• | DTC P0420 for the 1.2 L engine

• | DTC P0420 for the 1.4 L engine (L95)

• | DTC P0420 for the 1.6 L engine (LXT)

• | DTC P0420 for the 1.6 L engine (LXV)

P042E | Exhaust Gas Recirculation (EGR) Closed Position Performance | ECM | DTC P0403, P0404, P0405, P0406, or P042E
P0442 | Evaporative Emission (EVAP) System Small Leak Detected | ECM | DTC P0442 or P0456 for the 1.6 L engine (LXT) or DTC P0442 for the 1.6 L engine (LXV)
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM |

• | DTC P0443 for the 1.4 L engine (L95)

• | DTC P0443 for the 1.5 L engine

• | DTC P0443 for the 1.6 L engine (LXT)

• | DTC P0443 for the 1.6 L engine (LXV)

P0444 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Open | ECM | DTC P0444 or P0445
P0445 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Shorted | ECM | DTC P0444 or P0445
P0446 | Evaporative Emission (EVAP) Vent System Performance | ECM | DTC P0446 for the 1.6 L engine (LXT) or DTC P0446 for the 1.6 L engine (LXV)
P0449 | Evaporative Emission (EVAP) Vent Solenoid Control Circuit | ECM | DTC P0449 for the 1.6 L engine (LXT) or DTC P0449 for the 1.6 L engine (LXV)
P0451 | Fuel Tank Pressure (FTP) Sensor Performance | ECM | DTC P0451 or P0454 for the 1.6 L engine (LXT) or DTC P0451 or P0454 for the 1.6 L engine (LXV)
P0452 | Fuel Tank Pressure (FTP) Sensor Circuit Low Voltage | ECM | DTC P0452 or P0453 for the 1.6 L engine (LXT) or DTC P0452 or P0453 for the 1.6 L engine (LXV)
P0453 | Fuel Tank Pressure (FTP) Sensor Circuit High Voltage | ECM | DTC P0452 or P0453 for the 1.6 L engine (LXT) or DTC P0452 or P0453 for the 1.6 L engine (LXV)
P0454 | Fuel Tank Pressure (FTP) Sensor Intermittent | ECM | DTC P0451 or P0454 for the 1.6 L engine (LXT) or DTC P0451 or P0454 for the 1.6 L engine (LXV)
P0455 | Evaporative Emission (EVAP) System Large Leak Detected | ECM | DTC P0455 for the 1.6 L engine (LXT) or DTC P0455 for the 1.6 L engine (LXV)
P0456 | Evaporative Emission (EVAP) System Very Small Leak Detected | ECM | DTC P0442 or P0456
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Open | ECM | DTC P0458 or P0459
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Shorted | ECM | DTC P0458 or P0459
P0461 | Fuel Level Sensor Circuit Performance | ECM | DTC P0461
P0462 | Fuel Level Sensor Circuit Low Voltage | ECM | DTC P0462
P0463 | Fuel Level Sensor Circuit High Voltage | ECM | DTC P0463
P0464 | Fuel Level Circuit Intermittent | ECM | DTC P0464
P0480 | Cooling Fan Relay 1 Control Circuit | ECM | DTC P0480 or P0481
P0481 | Cooling Fan Relay 2 Control Circuit | ECM | DTC P0480 or P0481
P0496 | Evaporative Emission (EVAP) System Continuous Purge Flow | ECM | DTC P0496 for the 1.6 L engine (LXT) or DTC P0496 for the 1.6 L engine (LXV)
P0498 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit Open | ECM | DTC P0498 or P0499
P0499 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit Shorted | ECM | DTC P0498 or P0499
P0502 | Vehicle Speed Sensor (VSS) Circuit | ECM |

• | DTC P0502 for the 1.4 L engine (L95)

• | DTC P0502 for the 1.5 L engine

• | DTC P0502 for the 1.6 L engine (LXT)

P0503 | Vehicle Speed Sensor (VSS) Circuit Intermittent | ECM | DTC P0503
P0505 | Idle Control System | ECM | DTC P0505
P0506 | Idle Speed Low | ECM |

• | DTC P0506 or P0507 for the 1.4 L engine (L95)

• | DTC P0506 or P0507 for the 1.6 L engine (LXT)

• | DTC P0506 or P0507 for the 1.6 L engine (LXV)

P0507 | Idle Speed High | ECM |

• | DTC P0506 or P0507 for the 1.4 L engine (L95)

• | DTC P0506 or P0507 for the 1.6 L engine (LXT)

• | DTC P0506 or P0507 for the 1.6 L engine (LXV)

P050B | Ignition Timing Performance | ECM | DTC P050B
P050D | Cold Start Rough Idle | ECM | DTC P050D
P0513 | Theft Deterrent Key Incorrect | ECM | DTC P0513
P0520 | Engine Oil Pressure (EOP) Sensor Circuit | ECM | DTC P0520
P0532 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit Low Voltage | ECM | DTC P0532 or P0533
P0533 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit High Voltage | ECM | DTC P0532 or P0533
P0562 | System Voltage Low | ECM, TCM | DTC P0562 DTC P0562
P0563 | System Voltage High | ECM, TCM | DTC P0563 DTC P0563
P0564 | Cruise Control Multi-function Switch Circuit | ECM | DTC P0564
P0565 | Cruise Control Switch Circuit | ECM | DTC P0565
P0567 | Cruise Control Resume Switch Circuit | ECM | DTC P0567
P0568 | Cruise Control Set Switch Circuit | ECM | DTC P0568
P0571 | Cruise Control Brake Switch 1 Circuit | ECM | DTC P0571
P0572 | Brake Switch Circuit 1 Low Voltage | ECM | DTC P0572 or P0573
P0573 | Brake Switch Circuit 1 High Voltage | ECM | DTC P0572 or P0573
P0575 | Cruise Control Switch Signal Circuit | ECM | DTC P0575
P0601 | Control Module Read Only Memory (ROM) | ECM |

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4 L engine (L95)

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5 L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6 L engine (LXT)

• | DTC P0601-P0604, P0606, P062F, P16F3, or P2610 for the 1.6 L engine (LXV)

P0601 | Transmission Control Module (TCM) Read Only Memory (ROM) | TCM | DTC P0601 or P1790
P0602 | Control Module Not Programmed | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6 L engine (LXT)

• | DTC P0601-P0604, P0606, P062F, P16F3, or P2610 for the 1.6 L engine (LXV)

P0603 | Control Module Long Term Memory Reset | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6 L engine (LXT)

• | DTC P0601-P0604, P0606, P062F, P16F3, or P2610 for the 1.6 L engine (LXV)

P0604 | Control Module Random Access Memory (RAM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2 L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6 L engine (LXT)

• | DTC P0601-P0604, P0606, P062F, P16F3, or P2610 for the 1.6 L engine (LXV)

P0604 | Control Module Random Access Memory (RAM) | TCM | DTC P0604
P0605 | Control Module Programming Read Only Memory (ROM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2 L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6 L engine (LXT)

P0606 | Control Module Internal Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6 L engine (LXT)

• | DTC P0601-P0604, P0606, P062F, P16F3, or P2610 for the 1.6 L engine (LXV)

P0607 | Control Module Performance | ECM |

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4 L engine (L95)

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5 L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6 L engine (LXT)

P0615 | Starter Relay Control Circuit | ECM | DTC P0615
P0621 | Generator L-Terminal Circuit | ECM | DTC P0621
P0622 | Generator F-Terminal Circuit | ECM | DTC P0622
P061B | Control Module Internal Performance | ECM | DTC P061B or P161B
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0628 or P0629
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0628 or P0629
P062F | Control Module Long Term Memory Performance | ECM | DTC P0601-P0604, P0606, P062F, P16F3, or P2610
P0630 | VIN Not Programmed or Mismatched - Engine Control Module (ECM) | ECM | DTC P0630
P0633 | Theft Deterrent Key Not Programmed | ECM | DTC P0633
P0641 | 5-Volt Reference 1 Circuit | ECM | DTC P0641 or P0651 for the 1.6 L engine (LXT) or DTC P0641, P0651, P0697, or P06A3 for the 1.6 L engine (LXV)
P0645 | Air Conditioning (A/C) Clutch Relay Control Circuit | ECM | DTC P0645
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit Low Voltage | ECM |

• | DTC P0650 or P1650 for the 1.2 L engine

• | DTC P0650 for the 1.6 L engine (LXT)

• | DTC P0650 for the 1.6 L engine (LXV)

P0651 | 5-Volt Reference 2 Circuit | ECM | DTC P0641 or P0651 for the 1.6 L engine (LXT) or DTC P0641, P0651, P0697, or P06A3 for the 1.6 L engine (LXV)
P0656 | Fuel Level Output Circuit | ECM | DTC P0656
P0660 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit | ECM | DTC P0660 for the 1.4 L engine (L95) or DTC P0660 for the 1.6 L engine (LXT)
P0661 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit Low Voltage | ECM | DTC P0661 or P0662
P0662 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit High Voltage | ECM | DTC P0661 or P0662
P0685 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685 for the 1.6 L engine (LXT) or DTC P0685, P0689, or P0690 for the 1.6 L engine (LXV)
P0689 | Engine Controls Ignition Relay Feedback Circuit Low Voltage | ECM | DTC P0685, P0689, or P0690
P0690 | Engine Controls Ignition Relay Feedback Circuit High Voltage | ECM | DTC P0685, P0689, or P0690
P0697 | 5-Volt Reference 3 Circuit | ECM | DTC P0641, P0651, P0697, or P06A3
P06A3 | 5-Volt Reference 4 Circuit | ECM | DTC P0641, P0651, P0697, or P06A3
P06B6 | Knock Sensor (KS) Module Performance | ECM | DTC P0324, P0326, or P06B6
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM |

• | DTC P0700 for the 1.4 L engine (L95)

• | DTC P0700 for the 1.6 L engine (LXT)

• | DTC P0700 for the 1.6 L engine (LXV)

P0703 | Brake Switch Circuit 2 | ECM | DTC P0703
P0705 | Transmission Range Sensor Circuit | TCM | DTC P0705
P0706 | Transmission Range (TR) Switch Performance | TCM | DTC P0706
P0711 | Transmission Fluid Temperature Sensor (TFT) Sensor Performance | TCM | DTC P0711
P0712 | Transmission Fluid Temperature Sensor Low Input | TCM | DTC P0712
P0713 | Transmission Fluid Temperature Sensor Circuit High input | TCM | DTC P0713
P0717 | Input Speed Sensor - No Signal | TCM | DTC P0717
P0722 | Output Speed Sensor Circuit No Signal | TCM | DTC P0722
P0727 | Engine Speed Signal Circuit | TCM | DTC P0727
P0741 | Torque Converter Clutch (TCC) System-Stuck Off | TCM | DTC P0741
P0742 | Torque Converter Clutch Circuit Stuck On | TCM | DTC P0742
P0743 | Torque Converter Clutch Circuit Electrical | TCM | DTC P0743
P0748 | Pressure Control Solenoid Electrical | TCM | DTC P0748
P0751 | Shift Solenoid 1 Performance or Stuck Off | TCM | DTC P0751
P0752 | Shift Solenoid 1 Performance Stuck On | TCM | DTC P0752
P0753 | Shift Solenoid 1 Electrical | TCM | DTC P0753
P0756 | Shift Solenoid 2 Performance or Stuck Off | TCM | DTC P0756
P0757 | Shift Solenoid (SS) 2 Performance Stuck On | TCM | DTC P0757
P0758 | Shift Solenoid 2 Electrical | TCM | DTC P0758
P0785 | Shift Timing Solenoid | TCM | DTC P0785 or P1710
P0787 | Shift Timing Solenoid Low Voltage | TCM | DTC P0787
P0788 | Shift Timing Solenoid High Voltage | ECM | DTC P0788
P0806 | Clutch Pedal Position (CPP) Sensor Performance | ECM | DTC P0806-P0808
P0807 | Clutch Pedal Position (CPP) Sensor Circuit Low Voltage | ECM | DTC P0806-P0808
P0808 | Clutch Pedal Position (CPP) Sensor Circuit High Voltage | ECM | DTC P0806-P0808
P080A | Clutch Pedal Position (CPP) Not Learned | ECM | DTC P080A
P0812 | Reverse Position Switch Circuit | ECM | DTC P0812
P0834 | Clutch Pedal Switch Circuit Low Voltage | ECM | DTC P0834
P0835 | Clutch Pedal Switch Circuit High Voltage | ECM | DTC P0835
P0851 | Park/Neutral Position (PNP) Switch Circuit Low Voltage | ECM | DTC P0851 or P0852
P0852 | Park/Neutral Position (PNP) Switch Circuit High Voltage | ECM | DTC P0851 or P0852
P0962 | Line Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0962
P0963 | Line Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0963
P0973 | Shift Solenoid (SS) 1 Control Circuit Low Voltage | TCM | DTC P0973
P0974 | Shift Solenoid (SS) 1 Control Circuit High Voltage | TCM | DTC P0974
P0976 | Shift Solenoid (SS) 2 Control Circuit Low Voltage | TCM | DTC P0976
P0977 | Shift Solenoid (SS) 2 Control Circuit High Voltage | TCM | DTC P0977
P1101 | Intake Air Flow System Performance | ECM | DTC P0068 or P1101
P1106 | Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1106 or P1107 for the 1.4 L engine (L95)

• | DTC P1106 or P1107 for the 1.5 L engine

• | DTC P1106 or P1107 for the 1.6 L engine (LXT)

P1107 | Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent Low Voltage | ECM |

• | DTC P1106 or P1107 for the 1.4 L engine (L95)

• | DTC P1106 or P1107 for the 1.5 L engine

• | DTC P1106 or P1107 for the 1.6 L engine (LXT)

P1111 | Intake Air Temperature (IAT) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1111 or P1112 for the 1.4 L engine (L95)

• | DTC P1111 or P1112 for the 1.5 L engine

• | DTC P1111 or P1112 for the 1.6 L engine (LXT)

P1112 | Intake Air Temperature (IAT) Sensor Circuit Intermittent Low Voltage | ECM |

• | DTC P1111 or P1112 for the 1.4 L engine (L95)

• | DTC P1111 or P1112 for the 1.5 L engine

• | DTC P1111 or P1112 for the 1.6 L engine (LXT)

P1114 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent Low Voltage | ECM |

• | DTC P1114 or P1115 for the 1.4 L engine (L95)

• | DTC P1114 or P1115 for the 1.5 L engine

• | DTC P1114 or P1115 for the 1.6 L engine (LXT)

P1115 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1114 or P1115 for the 1.4 L engine (L95)

• | DTC P1114 or P1115 for the 1.5 L engine

• | DTC P1114 or P1115 for the 1.6 L engine (LXT)

P1116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P1116
P1121 | Throttle Position (TP) Sensor Circuit Intermittent High Voltage | P1121 |

• | DTC P1121 or P1122 for the 1.4 L engine (L95)

• | DTC P1121 or P1122 for the 1.5 L engine

• | DTC P1121 or P1122 for the 1.6 L engine (LXT)

P1122 | Throttle Position (TP) Sensor Circuit Intermittent Low Voltage | ECM |

• | DTC P1121 or P1122 for the 1.4 L engine (L95)

• | DTC P1121 or P1122 for the 1.5 L engine

• | DTC P1121 or P1122 for the 1.6 L engine (LXT)

P1133 | HO2S Insufficient Switching Sensor 1 | ECM |

• | DTC P0133, P1133, or P1134 for the 1.4 L engine (L95)

• | DTC P1133 for the 1.6 L engine (LXT)

• | DTC P0133 or P1133 for the 1.6 L engine (LXV)

P1134 | HO2S Transition Time Ratio Sensor 1 | ECM | DTC P0133, P1133, or P1134 for the 1.4 L engine (L95) or DTC P1134 for the 1.6 L engine (LXT)
P1137 | HO2S Circuit Low Voltage During Power Enrichment Sensor 1 | ECM | DTC P1137 or P1166
P1138 | HO2S Circuit High Voltage During Diesel Fuel Cut-Off (DFCO) Sensor 1 | ECM | DTC P1138 or P2297
P1166 | HO2S Circuit Low Voltage During Power Enrichment Sensor 2 | ECM | DTC P1166 for the 1.4 L engine (L95) or DTC P1137 or P1166 for the 1.6 L engine (LXT)
P1167 | HO2S Circuit High Voltage During Decel Fuel Cut-Off (DFCO) Sensor 1 | ECM | DTC P1167 for the 1.4 L engine (L95)
P1171 | HO2S Circuit Low Voltage During Power Enrichment Sensor 1 | ECM | DTC P1171
P1320 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P1320
P1321 | Crankshaft Position (CKP) Reluctor Wheel Performance | ECM | DTC P1321
P1336 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P1336
P1380 | Misfire Detected - Rough Road Data Not Available | ECM | DTC P1380 or P1381 for the 1.4 L engine (L95) or DTC P1380 or P1381 for the 1.6 L engine (LXT)
P1381 | Misfire Detected - No Communication With Brake Control Module | ECM | DTC P1380 or P1381 for the 1.4 L engine (L95) or DTC P1380 or P1381 for the 1.6 L engine (LXT)
P1390 | Wheel Speed Sensor Circuit | ECM | DTC P1390 or P1396
P1391 | Rough Road Sensor Performance | ECM | DTC P1391, P1392, or P1393 for the 1.4 L engine (L95 or DTC P1391, P1392, or P1393 for the 1.6 L engine (LXT)
P1392 | Rough Road Sensor Circuit Low Voltage | ECM | DTC P1391, P1392, or P1393 for the 1.4 L engine (L95 or DTC P1391, P1392, or P1393 for the 1.6 L engine (LXT)
P1393 | Rough Road Sensor Circuit High Voltage | ECM | DTC P1391, P1392, or P1393 for the 1.4 L engine (L95 or DTC P1391, P1392, or P1393 for the 1.6 L engine (LXT)
P1396 | Wheel Speed Sensor Circuit w/o ABS | ECM |

• | DTC P1390 or P1396 for the 1.2 L engine

• | DTC P1396 or P1397 for the 1.4 L engine (L95)

• | DTC P1396 or P1397 for the 1.6 L engine (LXT)

P1397 | Wheel Speed Sensor Circuit w/ABS | ECM | DTC P1396 or P1397 for the 1.4 L engine (L95) or DTC P1396 or P1397 for the 1.6 L engine (LXT)
P1400 | Cold Start Emission Reduction Control System | ECM | DTC P1400
P1402 | Exhaust Gas Recirculation (EGR) Flow Insufficient | ECM | DTC P0400, P0401, P0402, or P1402
P1404 | Exhaust Gas Recirculation (EGR) Closed Position Performance | ECM | DTC P0404-P0406, P042E, or P1404 for the 1.4 L engine (L95)
P1516 | Throttle Actuator control (TAC) Module Throttle Actuator Position Performance | ECM | DTC P1516, P2101, or P2119 for the 1.6 L engine (LXT) or DTC P1516, P2101, P2119, or P2176 for the 1.6 L engine (LXV)
P1601 | Lost Communication with TCM | ECM | DTC P1601 for the 1.4 L engine (L95) or DTC P1601 for the 1.5 L engine
P1610 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P1610 or P1611
P1611 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P1610 or P1611
P161B | Control Module Torque Performance | ECM | DTC P061B or P161B
P1626 | Lost Communication with Theft Deterrent Control Module | ECM | DTC P1626
P1631 | Theft Deterrent Fuel Enable Signal Not Correct | ECM | DTC P1631
P1650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4 L engine (L95) or DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5 L engine
P1655 | Control Module Internal Performance | ECM | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4 L engine (L95) or DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5 L engine
P1682 | Ignition 1 Switch Circuit 2 | ECM | DTC P1682
P16F3 | Control Module Redundant Memory Performance | ECM | DTC P0601-P0604, P0606, P062F, P16F3, or P2610
P1701 | Engine Coolant Temperature (ECT) Sensor Circuit | TCM | DTC P1701 or P1792
P1702 | Engine Torque Signal Error | TCM | DTC P1702
P1710 | Timing Solenoid Electrical | TCM | DTC P0785 or P1710
P1781 | Engine Torque Signal Error | TCM | DTC P1781
P1790 | Internal Control Module Memory Checksum Error | TCM | DTC P0601 or P1790
P1791 | Throttle Position (TP) Sensor Circuit | TCM | DTC P1791
P1792 | Engine Coolant Signal | TCM | DTC P1701 or P1792
P2076 | Intake Manifold Tuning (IMT) Valve Position Sensor Performance | ECM | DTC P2076, P2077, or P2078
P2077 | Intake Manifold Tuning (IMT) Valve Position Sensor Circuit Low Voltage | ECM | DTC P2076, P2077, or P2078
P2078 | Intake Manifold Tuning (IMT) Valve Position Sensor Circuit High Voltage | ECM | DTC P2076, P2077, or P2078
P2096 | Post Catalyst Fuel Trim System Low Limit Bank 1 | ECM | DTC P2096 or P2097
P2097 | Post Catalyst Fuel Trim System High Limit Bank 1 | ECM | DTC P2096 or P2097
P2101 | Throttle Actuator Position Performance | ECM | DTC P1516, P2101, or P2119 for the 1.6 L engine (LXT) or DTC P1516, P2101, P2119, or P2176 for the 1.6 L engine (LXV)
P2104 | Throttle Actuator Control (TAC) System - Forced Engine Idle | ECM | DTC P2104, P2105, P2106, or P2110
P2105 | Throttle Actuator Control (TAC) System - Forced Engine Shutdown | ECM | DTC P2104, P2105, P2106, or P2110
P2106 | Throttle Control System Performance - Throttle Limitation Active | ECM | DTC P2104, P2105, P2106, or P2110
P2110 | Throttle Actuator Control (TAC) System - Forced Limited Engine Speed | ECM | DTC P2104, P2105, P2106, or P2110
P2119 | Throttle Closed Position Performance | ECM | DTC P1516, P2101, or P2119 for the 1.6 L engine (LXT) or DTC P1516, P2101, P2119, or P2176 for the 1.6 L engine (LXV)
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 1.6 L engine (LXT) or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 1.6 L engine (LXV)
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 1.6 L engine (LXT) or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 1.6 L engine (LXV)
P2125 | Accelerator Pedal Position (APP) Sensor 2 Circuit | ECM | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 1.6 L engine (LXT) or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 1.6 L engine (LXV)
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 1.6 L engine (LXT) or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 1.6 L engine (LXV)
P2135 | Throttle Position (TP) Sensor 1-2 Correlation | ECM | DTC P0122, P0123, P0222, P0223, or P2135 for the 1.6 L engine (LXT) or DTC P0121-P0123, P0222, P0223, or P2135 for the 1.6 L engine (LXV)
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 1.6 L engine (LXT) or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 1.6 L engine (LXV)
P2176 | Minimum Throttle Position Not Learned | ECM | DTC P1516, P2101, P2119, or P2176
P2187 | Fuel Trim System Lean at Idle | ECM | DTC P0171, P0172, P2187, or P2188
P2188 | Fuel Trim System Rich at Idle | ECM | DTC P0171, P0172, P2187, or P2188
P2270 | HO2S Signal Stuck Lean Sensor 2 | ECM | DTC P2270
P2271 | HO2S Signal Stuck Rich Sensor 2 | ECM | DTC P2271
P2282 | Intake Manifold Air Leak | ECM | DTC P2282
P2297 | HO2S Circuit High Voltage during Decel Fuel Cut-Off (DFCO) Sensor 2 | ECM | DTC P2297 for the 1.4 L engine (L95) or DTC P1138 or P2297 for the 1.6 L engine (LXT)
P2544 | Transmission Torque Request Circuit | ECM | DTC P2544
P2610 | Control Module Ignition Off Timer Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6 L engine (LXT)

• | DTC P0601-P0604, P0606, P062F, P16F3, or P2610 for the 1.6 L engine (LXV)

P2769 | Torque Converter Clutch (TCC) Control Circuit Low Voltage | TCM | DTC P2769
P2770 | Torque Converter Clutch (TCC) Control Circuit High Voltage | TCM | DTC P2770
P2A00 | HO2S Performance Sensor 1 | ECM | DTC P2A00
P2A01 | HO2S Performance Sensor 2 | ECM | DTC P2A01
U0073 | Control Module Communication Bus Off | IPC, TDM | DTC U0073
U100 | Lost Comminication with ECM | IPC | DTC U0100-U0299
U0101 | Lost Communication with Transmission Control Module (TCM) | TCM | DTC U0100-U0299
U0155 | Lost Communication with IPC | TDM | DTC U0100-U0299
U0401 | Invalid Data Received from ECM/PCM | TCM | DTC U0401
U2105 | CAN Bus Error | TCM | DTC U2105