For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the crankshaft position (CKP) sensor electrical connector.
3. Remove the CKP sensor bolt.
4. Remove the CKP sensor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the CKP sensor with the bolt.

Tighten
Tighten the CKP sensor bolt to 6.5 N·m (58 lb in).

2. Connect the CKP sensor electrical connector.
3. Connect the negative battery cable.