For 1990-2009 cars

Checks | Actions
--- | ---
Check the tires for proper inflation pressures and normal tread wear. | Inflate the tires to the proper tire pressure. Replace the tires as needed.
Check the wheel bearings for looseness. | Tighten the axle nut to the proper specification. Replace the strut wheel bearing as needed.
Check for loose ball joints and tie rod ends. | Replace the ball joints and the tie rods.
Check the runout of the wheels and the tires. | Measure and correct the tire runout.
Check the vehicle trim heights. | Correct the trim heights. Make the correction before adjusting the toe.
Check for loose rack and pinion mounting. | Tighten the mounting brackets for the rack and pinion assembly.
Check for improperly operating struts. | Replace the strut assembly.
Check for loose control arms. | Tighten the control arm attachment bolts. Replace the control arm bushings as needed.