For 1990-2009 cars

### Removal Procedure

1. Remove the rear cushion. Refer to Rear Seat Cushion Replacement .
2. Remove the bolts that seat back.
3. Remove the rear seat back by pulling the base of the seat back out and sliding the seat back up.

### Installation Procedure

1. Insert the rear seat back by inserting the metal loops over the hooks.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear seat back with the bolts.

Tighten
Tighten the rear seat back bolt to 25 N·m (18 lb ft).

3. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .