For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the seal trim. Refer to Door Water Deflector Replacement .
3. Disconnect the inside door handle and the lock rods.
4. Disconnect the outside door handle and the lock rods.
5. Remove the bolts and the guide rail.
6. Remove the screws and the front door lock.
7. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Connect the inside door handle and the lock rods.
3. Connect the outside door handle and the lock rods.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the front door lock with the screws.

Tighten
Tighten the front door lock screws to 8 N·m (71 lb in).

5. Install the guide rail with the bolts.

Tighten
Tighten the guide rail bolts to 7 N·m (62 lb in).

6. Install the seal trim. Refer to Door Water Deflector Replacement .
7. Connect the negative battery cable.