For 1990-2009 cars

## Door Inside Handle Replacement Notchback

### Removal Procedure

1. Remove the water deflector. Refer to Door Water Deflector Replacement.
2. Remove the screw securing the door handle to the door.
3. Disconnect the inside door handle and the lock rods.

### Installation Procedure

1. Connect the inside door handle and the lock rods.
2. Insert the inside door handle into the slots in the door.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the inside door handle screw and tighten to 3 N·m (27 lb in).
4. Install the water deflector. Refer to Door Water Deflector Replacement.

## Door Inside Handle Replacement Hatchback

### Removal Procedure

1. Remove the door seal trim. Refer to Door Water Deflector Replacement.
2. Remove the screw securing the door handle to the door.
3. Disconnect the inside door handle and the lock rods.

### Installation Procedure

1. Connect the inside door handle and the lock rods.
2. Insert the inside door handle into the slots in the door.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the inside door handle screw and tighten to 3 N·m (27 lb in).
4. Install the door seal trim. Refer to Door Water Deflector Replacement.