For 1990-2009 cars

### Removal Procedure

1. Remove the floor console. Refer to Front Floor Console Replacement.
2. Disconnect the select and shift control cable. Refer to Shift Control Cable Replacement .
3. Remove the gear shift control lever bolts and assembly.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the gear shift control lever assembly and bolts (1).

Tighten
Tighten the bolts to 4-7 N·m (35-62 lb in).

2. Adjust the select cables. Refer to Shift Control Cable Replacement .
3. Connect the select and shift control cable. Refer to Shift Control Cable Replacement .
4. Install the floor console. Refer to Front Floor Console Replacement.