For 1990-2009 cars

## Clutch Pedal Replacement Hydraulic

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the return spring from the clutch pedal.
3. Remove the nut, the washer, and the pedal mounting shaft.
4. Remove the locking clip and push rod fixing pin.
5. Remove the push rod from the clutch pedal.
6. Remove the clutch pedal.

### Installation Procedure

1. Install the clutch pedal.
2. Coat the push rod with multi-purpose grease.
3. Install the push rod to the clutch pedal.
4. Install the locking clip and push rod fixing pin.
5. Coat the pedal mounting shaft with multi-purpose grease.

Notice: Refer to Fastener Notice in the Preface section.

6. Install the nut, the washer, and the pedal mounting shaft.

Tighten
Tighten the nut to 20 N·m (15 lb ft).

7. Connect the return spring to the clutch pedal.
8. Connect the negative battery cable.

## Clutch Pedal Replacement Cable

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the clutch cable. Refer to Clutch Cable Replacement .
2. Remove the clutch pedal bracket mounting bolts from the cowl.
3. Release the clutch pedal return spring.
4. Remove the clutch pedal shaft nut.
5. Remove the clutch pedal shaft.
6. Remove the clutch pedal from the mounting bracket.
7. Remove the clutch pedal mounting shaft bushings.
8. Remove the clutch pedal return spring.

### Installation Procedure

Important: Be sure to coat the clutch pedal shaft, the bushings and the spring with grease.

1. Install the clutch pedal return spring.
2. Install the clutch pedal mounting shaft bushings.
3. Install the clutch pedal to the mounting bracket.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the clutch pedal shaft.
5. Install the clutch pedal shaft nut.

Tighten
Tighten the clutch pedal mounting shaft nut to 20 N·m (15lb ft).

6. Re-attach the clutch pedal return spring to the clutch pedal.
7. Install the clutch cable. Refer to Clutch Cable Replacement .
8. Adjust the clutch cable. Refer to Clutch Assembly Adjustment .