For 1990-2009 cars

## Inline Harness Connector End Views Notchback

Table 1: | C105 Engine Harness to ECM Harness
Table 2: | C204 I/P Harness to Engine Harness
Table 3: | C205 I/P Harness to Engine Harness (MT34)
Table 4: | C206 TCM to I/P Harness
Table 5: | C207 Front Harness to I/P Harness (RHD)
Table 6: | C207 Front Harness to I/P Harness (LHD)
Table 7: | C208 I/P Harness to Front Harness (LHD)
Table 8: | C209 Front Harness to I/P Harness (LHD)
Table 9: | C210 Roof Harness to I/P Harness
Table 10: | C211 I/P Harness to Floor Harness (RHD)
Table 11: | C212 I/P Harness to Floor Harness (LHD)
Table 12: | C212 I/P Harness to Floor Harness (RHD)
Table 13: | C213 I/P Harness to Floor Harness (RHD)
Table 14: | C213 I/P Harness to Floor Harness (LHD)
Table 15: | C214 I/P Harness to Floor Harness (LHD)
Table 16: | C214 I/P Harness to Floor Harness (RHD)
Table 17: | C215 Air Bag Harness to I/P Harness (MT34)
Table 18: | C216 Air Bag Harness to I/P Harness
Table 19: | C217 I/P Harness to HVAC Harness
Table 20: | C218 I/P Harness to Floor Harness (RHD)
Table 21: | C219 I/P Harness to Floor Harness
Table 22: | C220 I/P Harness to Floor Harness (RHD)
Table 23: | C221 Front Harness to Floor Harness (RHD)
Table 24: | C351 Body Harness to Left Front Door Harness
Table 25: | C361 Body Harness to Right Front Door Harness
Table 26: | C371 Body Harness to Left Rear Door Harness
Table 27: | C381 Body Harness to Left Rear Door Harness
Table 28: | C401 Floor Harness to Trunk Harness
Table 29: | C402 Trunk Lid Harness to Floor Harness
Table 30: | C415 Rear Harness to Left Tail Lamp Jumper
Table 31: | C416 Rear Harness to Right Tail Lamp Jumper (Notchback)
Table 32: | C417 Rear Harness to Marker Lamp Jumper

#### C105 Engine Harness to ECM Harness

Connector Part Information |

• | KET MG 651068

• | 3-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641071-1

• | 3-Way M 090-II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | YE | -- | Serial Data Signal | 1 | YE | -- | Serial Data Signal
2 | PU | -- | Serial Data Signal | 2 | PU | -- | Serial Data Signal
3 | BK | -- | Ground | 3 | BK | -- | Ground

#### C204 I/P Harness to Engine Harness

Connector Part Information |

• | KET MG 651350

• | 18-Way F 090-II (WH)

Connector Part Information

• | KET MG 641353

• | 18-Way M 090-II (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | D-GN/WH | -- | Vehicle Speed Sensor Signal | 1 | D-GN/WH | -- | Vehicle Speed Sensor Signal
2 | WH | -- | Tachometer Signal | 2 | WH | -- | Tachometer Signal
3 | BN | -- | Charge Indicator Lamp Output | 3 | BN | -- | Charge Indicator Lamp Output
4 | BN/WH | -- | Check Engine Indicator Lamp Output | 4 | BN/WH | -- | Check Engine Indicator Lamp Output
5 | BN | -- | Ignition 2 Voltage | 5 | BN | -- | Ignition 2 Voltage
6 | YE (M/T) | -- | Ignition Switch Output - Crank | 6 | YE | -- | Ignition Switch Output - Crank
PU (A/T) | --
7 | D-GN | -- | Coolant Temperature Sensor Signal | 7 | D-GN | -- | Coolant Temperature Sensor Signal
8 | D-BU | -- | Fuel Gage Sensor Signal | 8 | D-BU | -- | Fuel Gage Sensor Signal
9 | L-BU | -- | Fuel Gage Sensor Ground | 9 | L-BU | -- | Fuel Gage Sensor Ground
10 | L-BU | -- | Evaporator Temperature Sensor Signal | 10 | L-BU | -- | Evaporator Temperature Sensor Signal
11 | D-BU | -- | Low Reference | 11 | D-BU | -- | Low Reference
12 | BN | -- | Oil Pressure Switch Signal | 12 | BN | -- | Oil Pressure Switch Signal
BN | -- | Oil Pressure Switch Signal
13 | BK/WH | -- | Serial Data | 13 | BK/WH | -- | Serial Data
14 | PU | -- | Fuel Gage Sensor Signal | 14 | PU | -- | Fuel Gage Sensor Signal
15 | D-GN/WH | -- | Air Conditioning Request Signal | 15 | D-GN/WH | -- | Air Conditioning Request Signal
16 | L-GN | -- | Backup Lamp Feed | 16 | L-GN | -- | Backup Lamp Feed
17 | -- | -- | Not Used | 17 | -- | -- | Not Used
18 | YE | -- | Hi Beam Indicator Feed | 18 | YE | -- | Hi Beam Indicator Feed

#### C205 I/P Harness to Engine Harness (MT34)

Connector Part Information |

• | MG611809

• | 18-Way F 090-II Series (WH)

Connector Part Information

• | MG621807

• | 36-Way M 090-II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | YE | -- | EVAP Vent Solenoid Control | 1 | YE | -- | EVAP Vent Solenoid Control
2 | BN/BK | -- | Fuel Tank Pressure Sensor Signal | 2 | BN/BK | -- | Fuel Tank Pressure Sensor Signal
3 | OG/BK | -- | Fuel Tank Pressure Sensor Signal 5-Volt Reference | 3 | OG/BK | -- | Fuel Tank Pressure Sensor Signal 5-Volt Reference
4 | PU | -- | Stop Lamp Switch Output | 4 | PU | -- | Stop Lamp Switch Output
5 | GY | -- | Cruise Control Switch Signal | 5 | GY | -- | Cruise Control Switch Signal
6 | YE | -- | Cruise Indicator Control | 6 | YE | -- | Cruise Indicator Control
7 | L-BU | -- | CPP Switch Signal | 7 | L-BU | -- | CPP Switch Signal
8 | GY | -- | 5-Volt Reference | 8 | GY | -- | 5-Volt Reference
9 | GY | -- | 5-Volt Reference | 9 | GY | -- | 5-Volt Reference
10 | BU | -- | APP Sensor 1 Signal | 10 | BU | -- | APP Sensor 1 Signal
11 | OG/BK | -- | Low Reference | 11 | WH | -- | Low Reference
12 | BN | -- | Low Reference | 12 | BN | -- | Low Reference
13 | L-BU | -- | APP Sensor 2 Signal | 13 | L-BU | -- | APP Sensor 2 Signal
14 | L-BU | -- | Stop Lamp Switch Output | 14 | L-BU | -- | Stop Lamp Switch Output
15-18 | -- | -- | Not Used | 15-18 | -- | -- | Not Used

#### C206 TCM to I/P Harness

Connector Part Information |

• | KET MG 651110-5

• | 10-Way F 090-II Series (BK)

Connector Part Information

• | KET MG 641113-5

• | 10-Way M 090-II Series (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | RD/WH | -- | Battery Positive Voltage | 1 | RD/WH | -- | Battery Positive Voltage
2 | BN | -- | Shift Solenoid Feed | 2 | BN | -- | Shift Solenoid Feed
3 | L-GN | -- | Back-Up Lamp Feed | 3 | L-GN | -- | Back-Up Lamp Feed
4 | GN/WH | -- | Brake Transmission Shift Interlock Solenoid Feed | 4 | GN/WH | -- | Brake Transmission Shift Interlock Solenoid Feed
5 | L-BU | -- | Stop Lamp Feed | 5 | L-BU | -- | Stop Lamp Feed
6 | BK/WH | -- | Serial Data | 6 | BK/WH | -- | Serial Data
7 | D-GN/WH | -- | Vehicle Speed Signal | 7 | D-GN/WH | -- | Vehicle Speed Signal
8 | PK | -- | Ignition 2 Voltage | 8 | BN | -- | Ignition 2 Voltage
9 | PK | -- | Ignition 1 Voltage | 9 | PK | -- | Ignition 1 Voltage
10 | YE | -- | Transmission Auxiliary Hold Signal | 10 | YE | -- | Transmission Auxiliary Hold Signal

#### C207 Front Harness to I/P Harness (RHD)

Connector Part Information |

• | KET MG 651926

• | 4-Way F 312-II Series (WH)

Connector Part Information

• | KET MG 641928

• | 4-Way M 312-II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | RD/BK | -- | Battery Positive Voltage | 1 | RD/BK | -- | Battery Positive Voltage
2 | RD/BK | -- | Battery Positive Voltage | 2 | RD/BK | -- | Battery Positive Voltage
3 | RD/BK | -- | Battery Positive Voltage | 3 | RD/BK | -- | Battery Positive Voltage
4 | RD/WH | -- | Battery Positive Voltage | 4 | RD/WH | -- | Battery Positive Voltage

#### C207 Front Harness to I/P Harness (LHD)

Connector Part Information |

• | MG653012-4

• | 12-Way F 090-II Series (GY)

Connector Part Information

• | MG643009-4

• | 12-Way M 090-II Series (GY)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | L-BU | -- | Stop Lamp Switch Output | 1 | L-BU | -- | Stop Lamp Switch Output
2 | GN | -- | Headlamp Leveling | 2 | GN | -- | Headlamp Leveling
L-GN | -- | SIR | L-GN | -- | SIR
3 | PK/BK | -- | Hood Open Signal | 3 | PK/BK | -- | Hood Open Signal
4 | YE | -- | Siren Control | 4 | YE | -- | Siren Control
5 | BK/WH | -- | Serial Data | 5 | BK/WH | -- | Serial Data
6 | GN/WH | -- | Front Fog Lamp Relay Control | 6 | GN/WH | -- | Front Fog Lamp Relay Control
7 | YE | -- | Front Fog Relay output | 7 | YE | -- | Front Fog Relay output
8 | L-GN | -- | ABS Indicator Control | 8 | L-GN | -- | ABS Indicator Control
9 | YE/BK | -- | SIR | 9 | YE/BK | -- | SIR
10 | YE | -- | Ambient Temp Signal | 10 | YE | -- | Ambient Temp Signal
11 | L-GN/BK | -- | Ground | 11 | BK | -- | Ground
12 | YE | -- | SIR | 12 | YE | -- | SIR

#### C208 I/P Harness to Front Harness (LHD)

Connector Part Information |

• | HS015-20105

• | 20-Way F (OG)

Connector Part Information

• | HS011-20105

• | 20-Way M (OG)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BN | -- | Wiper Relay Park Signal | 1 | BN | -- | Wiper Relay Park Signal
2 | D-GN | -- | Front Wiper High Signal | 2 | D-GN | -- | Front Wiper High Signal
3 | D-BU | -- | Hazard Switch | 3 | D-BU | -- | Hazard Switch
4 | L-BU | -- | Headlamp Hi Relay Control | 4 | L-BU | -- | Headlamp Hi Relay Control
5 | WH | -- | Illumination Relay Coil Supply | 5 | WH | -- | Illumination Relay Coil Supply
6 | BN/WH | -- | Illumination Relay Output | 6 | BN/WH | -- | Illumination Relay Output
7 | L-GN/BK | -- | Headlamp Low Relay Output | 7 | L-GN/BK | -- | Headlamp Low Relay Output
8 | PK | -- | Ignition 1 Voltage | 8 | PK | -- | Ignition 1 Voltage
9 | PU | -- | Front Wiper Motor Voltage | 9 | PU | -- | Front Wiper Motor Voltage
10 | PK | -- | Ignition 2 Voltage | 10 | PK | -- | Ignition 2 Voltage
11 | BN | -- | Brake Indicator Control | 11 | BN | -- | Brake Indicator Control
12 | PU | -- | Ignition 1 Voltage | 12 | PU | -- | Ignition 1 Voltage
13 | BN/WH | -- | High Beam Indicator Control | 13 | BN/WH | -- | High Beam Indicator Control
14 | BN | -- | Horn Relay Output | 14 | BN | -- | Horn Relay Output
15 | PK | -- | Front Washer Pump Signal | 15 | PK | -- | Front Washer Pump Signal
16 | RD/BK | -- | Battery Positive Voltage | 16 | RD/WH | -- | Battery Positive Voltage
17 | PK | -- | Ignition 1 Voltage | 17 | PK | -- | Ignition 1 Voltage
18 | RD/WH | -- | Battery Positive Voltage | 18 | RD/WH | -- | Battery Positive Voltage
19 | L-BU | -- | Left Turn Signal | 19 | L-BU | -- | Left Turn Signal
20 | WH | -- | Headlamp Low Relay Control | 20 | WH | -- | Headlamp Low Relay Control

#### C209 Front Harness to I/P Harness (LHD)

Connector Part Information |

• | KET MG 651926

• | 4-Way F 312-II Series (BK)

Connector Part Information

• | KET MG 641928

• | 4-Way M 312-II Series (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | RD/BK | -- | Battery Positive Voltage | 1 | RD/BK | -- | Battery Positive Voltage
2 | RD/BK | -- | Battery Positive Voltage | 2 | RD/BK | -- | Battery Positive Voltage
3 | RD/BK | -- | Battery Positive Voltage | 3 | RD/BK | -- | Battery Positive Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used

#### C210 Roof Harness to I/P Harness

Connector Part Information |

• | 936092-4

• | 10-Way F (BN)

Connector Part Information

• | 936129-1

• | 10-Way M (NA)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BK | -- | Ground | 1 | BK | -- | Ground
2 | BN | -- | Ignition 3 | 2 | BN | -- | Ignition 3
3 | RD/WH | -- | Fuse Output | 3 | RD/WH | -- | Fuse Output
4 | GY | -- | Speaker Return - Left Front | 4 | GY | -- | Speaker Return - Left Front
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | GY | -- | Interior Lamp Control | 6 | GY | -- | Interior Lamp Control
7 | RD/WH | -- | Battery Positive Voltage | 7 | RD/WH | -- | Battery Positive Voltage
8 | BN | -- | Speaker Feed - Left Front | 8 | BN | -- | Speaker Feed - Left Front
9 | PU/WH | -- | Overspeed Signal (LHD) | 9 | PU/WH | -- | Overspeed Signal (LHD)
10 | PU/WH | -- | Overspeed Signal (LHD) | 10 | PU/WH | -- | Overspeed Signal (LHD)

#### C211 I/P Harness to Floor Harness (RHD)

Connector Part Information |

• | KET MG 622244-3

• | 15-Way F 090-II Series (YE)

Connector Part Information

• | KET MG 622244-3

• | 15-Way M 090-II Series (YE)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | L-GN/BK | -- | Power Window Relay Output | 3 | L-GN/BK | -- | Power Window Relay Output
4-6 | -- | -- | Not Used | 4-6 | -- | -- | Not Used
7 | L-GN/BK | -- | Power Window Relay Output | 7 | L-GN/BK | -- | Power Window Relay Output
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | BN | -- | Fuel Pump Relay Output | 9 | BN | -- | Fuel Pump Relay Output
10 | BN | -- | Wheel Speed Sensor Signal - Right Rear | 10 | BN | -- | Wheel Speed Sensor Signal - Right Rear
11 | WH | -- | Wheel Speed Sensor Return - Right Rear | 11 | WH | -- | Wheel Speed Sensor Return - Right Rear
12 | BN | -- | Wheel Speed Sensor Signal - Left Rear | 12 | BN | -- | Wheel Speed Sensor Signal - Left Rear
13 | OG | -- | Wheel Speed Sensor Return - Left Rear | 13 | OG | -- | Wheel Speed Sensor Return - Left Rear
14 | BN/WH | -- | Park Lamp Feed - Right | 14 | BN/WH | -- | Park Lamp Feed - Right
15 | PU | -- | Park Lamp Feed - Left | 15 | PU | -- | Park Lamp Feed - Left

#### C212 I/P Harness to Floor Harness (LHD)

Connector Part Information |

• | KET MG 651044

• | 11-Way F (BU)

Connector Part Information

• | KET MG 641047

• | 11-Way M (BU)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | RD/WH | -- | Battery Voltage | 1 | RD/WH | -- | Battery Voltage
2 | OG | -- | Rear Fog Relay Output | 2 | OG | -- | Rear Fog Relay Output
3 | RD/WH | -- | Battery Voltage | 3 | RD/WH | -- | Battery Voltage
4 | OG | -- | Defog Relay Output | 4 | OG | -- | Defog Relay Output
5 | L-BU | -- | Stop Lamp Feed | 5 | L-BU | -- | Stop Lamp Feed
6 | OG | -- | Defog Relay Output | 6 | OG | -- | Defog Relay Output
OG | --
7 | D-BU | -- | Right Turn Signal | 7 | D-BU | -- | Right Turn Signal
8 | GY | -- | Power Mirror Motor Ground | 8 | GY | -- | Power Mirror Motor Ground
GY | --
9 | L-BU | -- | Left Turn Signal | 9 | L-BU | -- | Left Turn Signal
10 | L-GN | -- | Backup Lamp Voltage | 10 | L-GN | -- | Backup Lamp Voltage
11 | YE | -- | Ignition 1 Voltage | 11 | YE | -- | Ignition 1 Voltage

#### C212 I/P Harness to Floor Harness (RHD)

Connector Part Information |

• | KET MG 622244-3

• | 15-Way F 090-II Series (YE)

Connector Part Information

• | KET MG 622244-3

• | 15-Way M 090-II Series (YE)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | PK | -- | Ignition 1 Voltage | 1 | PK | -- | Ignition 1 Voltage
2 | D-GN/WH | -- | Front Fog Relay Control | 2 | D-GN/WH | -- | Front Fog Relay Control
D-GN/WH | --
3 | L-GN/BK | -- | Power Window Relay Output | 3 | L-GN/BK | -- | Power Window Relay Output
4 | BN | -- | Cigar Relay Control | 4 | BN | -- | Cigar Relay Control
5 | D-GN | -- | Dome Relay Control | 5 | D-GN | -- | Dome Relay Control
6 | YE | -- | HI Beam Indicator Control | 6 | YE | -- | HI Beam Indicator Control
7 | WH | -- | Illumination Relay Control | 7 | WH | -- | Illumination Relay Control
8 | PU | -- | Not Used | 8 | PU | -- | Not Used
9 | BN/WH | -- | Illumination Relay Output | 9 | BN/WH | -- | Illumination Relay Output
10 | D-GN | -- | Front Wiper High Speed | 10 | D-GN | -- | Front Wiper High Speed
11 | PK | -- | Ignition 1 Voltage | 11 | PK | -- | Ignition 1 Voltage
12 | YE | -- | Front Fog Relay Output | 12 | YE | -- | Front Fog Relay Output
13 | PK | -- | Ignition Voltage | 13 | PK | -- | Ignition Voltage
PK | --
14 | BN | -- | Horn Relay Output | 14 | BN | -- | Horn Relay Output
15 | PU | -- | Front Wiper Low Speed | 15 | PU | -- | Front Wiper Low Speed

#### C213 I/P Harness to Floor Harness (RHD)

Connector Part Information |

• | KET MG 651086-3

• | 20-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641089-3

• | 20-Way F 090-II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | OG | -- | Fog Lamp Feed - Rear | 1 | OG | -- | Fog Lamp Feed - Rear
2 | WH | -- | Courtesy Lamp Control | 2 | WH | -- | Courtesy Lamp Control
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | L-GN | -- | Back-Up Lamp Feed | 4 | L-GN | -- | Back-Up Lamp Feed
5 | RD/WH | -- | Battery Voltage | 5 | RD/WH | -- | Battery Voltage
6 | OG | -- | Heated Mirror Element Feed | 6 | OG | -- | Heated Mirror Element Feed
OG | --
7 | WH | -- | Door Lock Switch Signal | 7 | WH | -- | Door Lock Switch Signal
8 | L-BU | -- | Power Door Lock Relay Feed - Lock Coil | 8 | L-BU | -- | Power Door Lock Relay Feed - Lock Coil
9 | WH | -- | Courtesy Lamp Output | 9 | WH | -- | Courtesy Lamp Output
10 | L-BU | -- | Stop Lamp Feed | 10 | L-BU | -- | Stop Lamp Feed
11 | OG | -- | Defog Relay Output | 11 | OG | -- | Defog Relay Output
12 | L-BU | -- | Trunk Key Cylinder Switch Signal | 12 | PU | -- | Trunk Key Cylinder Switch Signal
13 | PU | -- | Door Key Lock Cylinder Switch Signal - Passenger | 13 | L-GN/RD | -- | Door Key Lock Cylinder Switch Signal - Passenger
14 | PU | -- | Door Key Lock Cylinder Switch Signal - Driver | 14 | BN/BK | -- | Door Key Lock Cylinder Switch Signal - Driver
15 | BN | -- | Trunk Release Relay Feed-Coil | 15 | BN | -- | Trunk Release Relay Feed-Coil
16 | OG/BK | -- | Trunk Lamp Output | 16 | GY/BK | -- | Trunk Lamp Output
17 | -- | -- | Not Used | 17 | -- | -- | Not Used
18 | YE | -- | Low Fuel Indicator Lamp Output | 18 | YE | -- | Low Fuel Indicator Lamp Output
19 | BN/WH | -- | Brake Warning Indicator Lamp Control | 19 | BN/WH | -- | Brake Warning Indicator Lamp Control
20 | BN/WH | -- | Seat Belt Switch Signal | 20 | BN/WH | -- | Seat Belt Switch Signal
21 | GY | -- | Power Mirror Motor Feed - Right Horizontal Motor - Left Direction | 21 | GY | -- | Power Mirror Motor Feed - Right Horizontal Motor - Left Direction
22 | PK | -- | Ignition 1 Voltage | 22 | PK | -- | Ignition 1 Voltage

#### C213 I/P Harness to Floor Harness (LHD)

Connector Part Information |

• | KET MG 611810-41

• | 20-Way F (WH)

Connector Part Information

• | KET MG 652426

• | 20-Way M (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | GY | -- | Door Lock Relay Output | 1 | GY | -- | Door Lock Relay Output
2 | BN | -- | Door Unlock Relay Output | 2 | BN | -- | Door Unlock Relay Output
3 | BN/WH | -- | Park Brake Signal | 3 | BN/WH | -- | Park Brake Signal
4 | BN/WH | -- | Seat Belt Switch Signal | 4 | BN/WH | -- | Seat Belt Switch Signal
5 | YE | -- | Low Fuel Indicator Control | 5 | YE | -- | Low Fuel Indicator Control
6-7 | -- | -- | Not Used | 6-7 | -- | -- | Not Used
8 | L-BU | -- | Door Lock Switch Signal | 8 | L-BU | -- | Door Lock Switch Signal
9 | WH | -- | Door Lock Switch Signal | 9 | WH | -- | Door Lock Switch Signal
10 | PU | -- | Tamper Switch Signal | 10 | PU | -- | Tamper Switch Signal
11 | PU | -- | Door Tamper Switch Signal - RH | 11 | L-GN/RD | -- | Door Tamper Switch Signal - RH
12 | PU | -- | Door Tamper Switch Signal - LH | 12 | BN/BK | -- | Door Tamper Switch Signal - LH
13 | BN | -- | Trunk Switch Signal | 13 | BN | -- | Trunk Switch Signal
14 | OG/BK | -- | Trunk Open Signal | 14 | GY/BK | -- | Trunk Open Signal
15 | PU | -- | Illumination Relay Output | 15 | PU | -- | Illumination Relay Output
16 | -- | -- | Not Used | 16 | -- | -- | Not Used
17 | WH | -- | Right Mirror Voltage | 17 | WH | -- | Right Mirror Voltage
18 | L-GN | -- | Right Mirror Voltage | 18 | L-GN | -- | Right Mirror Voltage
19 | YE | -- | Left Mirror Voltage | 19 | YE | -- | Left Mirror Voltage
20 | L-BU | -- | Left Mirror Voltage | 20 | L-BU | -- | Left Mirror Voltage

#### C214 I/P Harness to Floor Harness (LHD)

Connector Part Information |

• | KET MG 651044

• | 22-Way F (BK)

Connector Part Information

• | KET MG 641047

• | 22-Way M (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | L-BU | -- | Fuel Gage Sensor Ground | 1 | L-BU | -- | Fuel Gage Sensor Ground
2 | D-BU | -- | Fuel Gage Sensor Signal | 2 | D-BU | -- | Fuel Gage Sensor Signal
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | WH | -- | Courtesy Lamp Control | 4 | WH | -- | Courtesy Lamp Control
5 | WH | -- | Driver Door Courtesy Lamp Control | 5 | WH | -- | Driver Door Courtesy Lamp Control
6 | GN | -- | Radio Cassette | 6 | GN | -- | Radio Cassette
7 | BN | -- | Speaker Feed - LF | 7 | BN | -- | Speaker Feed - LF
8 | L-GN | -- | Speaker Feed - RF | 8 | L-GN | -- | Speaker Feed - RF
9 | GY | -- | Speaker Return - LF | 9 | GY | -- | Speaker Return - LF
10 | D-GN | -- | Speaker Return - RF | 10 | D-GN | -- | Speaker Return - RF
11 | BN | -- | Fuel Tank Pressure Signal | 11 | BN | -- | Fuel Tank Pressure Signal
12 | OG | -- | Fuel Tank Pressure 5-Volt Reference | 12 | OG | -- | Fuel Tank Pressure 5-Volt Reference
13 | PK | -- | Ignition 1 Voltage | 13 | PK | -- | Ignition 1 Voltage
14 | YE | -- | Undefined | 14 | YE | -- | Undefined
15-18 | -- | -- | Not Used | 15-18 | -- | -- | Not Used
19 | BN | -- | Speaker Feed - LR | 19 | BN | -- | Speaker Feed - LR
20 | YE | -- | Speaker Feed - LR | 20 | YE | -- | Speaker Feed - LR
21 | D-BU | -- | Speaker Feed - RR | 21 | D-BU | -- | Speaker Feed - RR
22 | L-BU | -- | Speaker Feed - RR | 22 | L-BU | -- | Speaker Feed - RR

#### C214 I/P Harness to Floor Harness (RHD)

Connector Part Information |

• | KET MG 651056-5

• | 10-Way F 090-II Series (BK)

Connector Part Information

• | KET MG 641059-5

• | 10-Way M 090-II Connector (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BN | -- | Power Door Lock Motor Feed - Unlock | 1 | BN | -- | Power Door Lock Motor Feed - Unlock
2 | L-BU | -- | Left Turn Signal | 2 | L-BU | -- | Left Turn Signal
3 | WH | -- | Headlamp Relay Control | 3 | WH | -- | Headlamp Relay Control
4 | YE | -- | Ignition 1 Voltage | 4 | YE | -- | Ignition 1 Voltage
5 | GY | -- | Power Door Lock Motor Feed - Lock | 5 | GY | -- | Power Door Lock Motor Feed - Lock
6 | D-BU | -- | Turn Signal Lamp Feed - Right Front | 6 | D-BU | -- | Turn Signal Lamp Feed - Right Front
7 | WH | -- | Power Mirror Motor Feed - Left Horizontal Motor - Right Direction | 7 | WH | -- | Power Mirror Motor Feed - Left Horizontal Motor - Right Direction
8 | L-GN | -- | Power Mirror Motor Feed - Left Vertical Motor - Down Direction | 8 | L-GN | -- | Power Mirror Motor Feed - Left Vertical Motor - Down Direction
9 | L-BU | -- | Power Mirror Motor Feed - Left Horizontal Motor - Left Direction | 9 | L-BU | -- | Power Mirror Motor Feed - Left Horizontal Motor - Left Direction
10 | YE | -- | Power Mirror Motor Feed - Left Vertical Motor - Up Direction | 10 | YE | -- | Power Mirror Motor Feed - Left Vertical Motor - Up Direction

#### C215 Air Bag Harness to I/P Harness (MT34)

Connector Part Information |

• | 368501-1

• | 4-Way F .070 MLC Series (WH)

Connector Part Information

• | 174929-1

• | 4-Way M .070 MLC Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | PU | -- | Front Discriminating Sensor - Left - High | 1 | PU | -- | Front Discriminating Sensor - Left - High
2 | RD | -- | Front Discriminating Sensor - Left - Low | 2 | RD | -- | Front Discriminating Sensor - Left - Low
3 | BK | -- | Front Discriminating Sensor - Right - High | 3 | BK | -- | Front Discriminating Sensor - Right - High
4 | GN | -- | Front Discriminating Sensor - Right - Low | 4 | GN | -- | Front Discriminating Sensor - Right - Low

#### C216 Air Bag Harness to I/P Harness

Connector Part Information |

• | KET MG 651068

• | 12-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641071

• | 12-Way M 090-II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | GY/BK | -- | Passenger Air Bag On Indicator Control (Advanced Air Bag) | 1 | GY/BK | -- | Passenger Air Bag On Indicator Control (Advanced Air Bag)
2 | L-BU | -- | Vehicle Speed Sensor Signal | 2 | L-BU | -- | Vehicle Speed Sensor Signal
3 | D-GN/WH | -- | Driver Information Center Switch Signal | 3 | GB/WH | -- | Driver Information Center Switch Signal
4 | YE | -- | Accessory Fuse | 4 | YE | -- | Accessory Fuse
5 | YE | -- | Accessory Fuse | 5 | YE | -- | Accessory Fuse
6 | L-GN | -- | SIR Chime Signal | 6 | L-GN | -- | SIR Chime Signal
7 | PK | -- | Ignition 1 Voltage | 7 | PK | -- | Ignition 1 Voltage
8 | L-BU | -- | Diagnostic Signal - SIR | 8 | YE/BK | -- | Diagnostic Signal - SIR
9 | BN | -- | SIR Indicator Lamp Control | 9 | BN | -- | SIR Indicator Lamp Control
10 | PK | -- | Ignition 1 Voltage (LHD) | 10 | PK | -- | Ignition 1 Voltage (LHD)
11 | D-GN | -- | Seat Belt Switch Signal | 11 | BN/WH | -- | Seat Belt Switch Signal
12 | D-GN/WH | -- | Passenger Air Bag Indicator Control | 12 | D-GN/WH | -- | Passenger Air Bag Indicator Control

#### C217 I/P Harness to HVAC Harness

Connector Part Information |

• | MG651006

• | 16-Way F 1809 Series (WH)

Connector Part Information

• | MG620397

• | 16-Way M Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | PU | -- | Windshield Wiper Motor Feed - High Speed | 1 | YE/BK | -- | Windshield Wiper Motor Feed - High Speed
2 | D-GN/WH | -- | Vehicle Speed Signal | 2 | L-GN | -- | Vehicle Speed Signal
3 | BN/WH | -- | Park Lamp Feed - Right | 3 | D-GN/WH | -- | Park Lamp Feed - Right
4 | BN/WH | -- | Instrument Panel Lamps Dimmer Module | 4 | D-GN/BK | -- | Instrument Panel Lamps Dimmer Module
5 | RD/WH | -- | Battery Voltage | 5 | WH/RD | -- | Battery Voltage
6 | BN | -- | Ignition 2 Voltage | 6 | YE/WH | -- | Ignition 2 Voltage
7 | WH | -- | Rear Defogger Relay Output - Coil | 7 | BN/RD | -- | Rear Defogger Relay Output - Coil
8 | GN/WH | -- | Air Conditioning Request Signal | 8 | YE/D-GN | -- | Air Conditioning Request Signal
9 | BK | -- | Outside Ambient Temperature Sensor Signal | 9 | D-BU/WH | -- | Outside Ambient Temperature Sensor Signal
10 | YE | -- | Outside Ambient Temperature Sensor Return | 10 | D-GN/YE | -- | Outside Ambient Temperature Sensor Return
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | BN | -- | Not Used | 12 | L-GN/RD | -- | Not Used
13 | BK | -- | Ground | 13 | BK | -- | Ground
14 | OG | -- | Ignition Switch Output - Ignition 3 | 14 | RD/WH | -- | Ignition Switch Output - Ignition 3
15 | -- | -- | Not Used | 15 | D-GN | -- | Fan Switch Signal
16 | -- | -- | Not Used | 16 | RD/YE | -- | PTC

#### C218 I/P Harness to Floor Harness (RHD)

Connector Part Information |

• | KET MG 611810-41

• | 20-Way F (WH)

Connector Part Information

• | KET MG 652426

• | 20-Way M (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | L-BU | -- | Fuel Gage Sensor Signal - Right | 1 | L-BU | -- | Fuel Gage Sensor Signal - Right
2 | D-BU | -- | Fuel Gage Sensor Signal - Left | 2 | D-BU | -- | Fuel Gage Sensor Signal - Left
3-8 | -- | -- | Not Used | 3-8 | -- | -- | Not Used
9 | D-GN | -- | Power Antenna Relay Feed-Coil | 9 | D-GN | -- | Power Antenna Relay Feed-Coil
10 | BN | -- | Speaker Feed - Left Front | 10 | BN | -- | Speaker Feed - Left Front
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | GY | -- | Speaker Return - Left Front | 12 | GY | -- | Speaker Return - Left Front
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | D-GN | -- | Speaker Return - Right Front | 14 | D-GN | -- | Speaker Return - Right Front
15 | L-GN | -- | Speaker Feed - Right Front | 15 | L-GN | -- | Speaker Feed - Right Front
16 | BN | -- | Speaker Feed - Left Rear | 16 | BN | -- | Speaker Feed - Left Rear
17 | YE | -- | Speaker Return - Left Rear | 17 | YE | -- | Speaker Return - Left Rear
18 | D-BU | -- | Speaker Feed - Right Rear | 18 | D-BU | -- | Speaker Feed - Right Rear
19 | L-BU | -- | Speaker Return - Right Rear | 19 | L-BU | -- | Speaker Return - Right Rear
20 | L-GN/BK | -- | Headlamp Low Relay Output | 20 | L-GN/BK | -- | Headlamp Low Relay Output

#### C219 I/P Harness to Floor Harness

Connector Part Information |

• | KET MG 651044

• | 8-Way F (BU)

Connector Part Information

• | KET MG 641047

• | 8-Way M (BU)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | YE | -- | Outside Ambient Temperature Sensor Return | 1 | YE | -- | Outside Ambient Temperature Sensor Return
2 | L-GN | -- | ABS Failure Indicator Lamp Output | 2 | L-GN | -- | ABS Failure Indicator Lamp Output
3 | YE | -- | Security Signal - Arm Alarm | 3 | YE | -- | Security Signal - Arm Alarm
4 | BK/WH | -- | Serial Data | 4 | BK/WH | -- | Serial Data
5 | BU | -- | Turn Signal Lamp Feed - Right Front | 5 | BU | -- | Turn Signal Lamp Feed - Right Front
6 | BK | -- | Ground | 6 | L-GN/BK | -- | Ground
7 | RD/WH | -- | Battery Voltage | 7 | RD/WH | -- | Battery Voltage
8 | PK/BK | -- | Hood Ajar Switch Signal | 8 | PK/BK | -- | Hood Ajar Switch Signal

#### C220 I/P Harness to Floor Harness (RHD)

Connector Part Information |

• | KET MG 651044

• | 22-Way F (BK)

Connector Part Information

• | KET MG 641047

• | 22-Way M (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BN | -- | Brake Warning Indicator Lamp Output | 1 | BN | -- | Brake Warning Indicator Lamp Output
2 | RD/BK | -- | Battery Voltage | 2 | RD/BK | -- | Battery Voltage
3 | PU | -- | Power Window Enable Relay Output - N.O. Contact | 3 | PU | -- | Power Window Enable Relay Output - N.O. Contact
4 | L-GN/BK | -- | Headlamp Low Relay Output | 4 | L-GN/BK | -- | Headlamp Low Relay Output
5 | WH | -- | Headlamp Relay Control | 5 | WH | -- | Headlamp Relay Control
6 | GN | -- | Headlamp Leveling Motor Feed | 6 | GN | -- | Headlamp Leveling Motor Feed
7 | YE | -- | Outside Ambient Temperature Sensor Return | 7 | YE | -- | Outside Ambient Temperature Sensor Return
8 | L-GN | -- | ABS Failure Indicator Lamp Output | 8 | L-GN | -- | ABS Failure Indicator Lamp Output
9 | PK/BK | -- | Hood Ajar Switch Signal | 9 | PK/BK | -- | Hood Ajar Switch Signal
10 | YE | -- | Security Signal - Arm Alarm | 10 | YE | -- | Security Signal - Arm Alarm
11 | L-GN/BK | -- | Outside Ambient Temperature Sensor Signal | 11 | L-GN/BK | -- | Outside Ambient Temperature Sensor Signal
12 | GN/WH | -- | Fog Lamp Relay Control | 12 | GN/WH | -- | Fog Lamp Relay Control
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | BN/WH | -- | Park Lamp Feed - Right | 14 | BN/WH | -- | Park Lamp Feed - Right
15 | L-BU | -- | Headlamp Relay Output - N.O. Contact | 15 | L-BU | -- | Headlamp Relay Output - N.O. Contact
16 | L-BU | -- | Stop Lamp Feed | 16 | L-BU | -- | Stop Lamp Feed
17 | BK/WH | -- | Serial Data | 17 | BK/WH | -- | Serial Data
18 | -- | -- | Not Used | 18 | -- | -- | Not Used
19 | WH | -- | Illumination Relay Control | 19 | WH | -- | Illumination Relay Control
20 | D-BU | -- | Turn Signal Lamp Feed - Right Front | 20 | D-BU | -- | Turn Signal Lamp Feed - Right Front
21 | L-BU | -- | Turn Signal Lamp Feed - Left Front | 21 | L-BU | -- | Turn Signal Lamp Feed - Left Front
22 | PK | -- | Windshield Washer Signal | 22 | PK | -- | Windshield Washer Signal

#### C221 Front Harness to Floor Harness (RHD)

Connector Part Information |

• | MG651044

• | 11-Way F (BU)

Connector Part Information

• | MG641047

• | 11-Way M (BU)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | PK | -- | Ignition 1 Voltage | 1 | PK | -- | Ignition 1 Voltage
2 | PK | -- | Ignition 1 Voltage | 2 | PK | -- | Ignition 1 Voltage
3 | YE | -- | Front Fog Relay output | 3 | YE | -- | Front Fog Relay output
4 | GN | -- | Windshield Wiper Motor High Speed | 4 | GN | -- | Windshield Wiper Motor High Speed
5 | PU | -- | Windshield Wiper Motor Low Speed | 5 | PU | -- | Windshield Wiper Motor Low Speed
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | BN | -- | Windshield Wiper Switch Signal - Pulse Delay | 7 | BN | -- | Windshield Wiper Switch Signal - Pulse Delay
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | BN | -- | Horn Relay Output | 9 | BN | -- | Horn Relay Output
10 | YE | -- | HI Beam Indicator Control | 10 | YE | -- | HI Beam Indicator Control
11 | PK | -- | Ignition 1 Voltage | 11 | PK | -- | Ignition 1 Voltage

#### C351 Body Harness to Left Front Door Harness

Connector Part Information |

• | KET MG 610692

• | 29-Way F Door (WH)

Connector Part Information

• | KET MG 620693

• | 29-Way M Door Connector (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | L-GN/BK | -- | Power Window Relay Output | 1 | L-GN/BK | -- | Power Window Relay Output
2 | D-BU | -- | Power Window Master Switch Output - Lockout | 2 | D-BU | -- | Power Window Master Switch Output - Lockout
3 | L-BU | -- | Power Window Master Switch Output - Pass Front Window - Up | 3 | L-BU | -- | Power Window Master Switch Output - Pass Front Window - Up
4 | BN | -- | Power Window Master Switch Output - Pass Front Window - Down | 4 | BN | -- | Power Window Master Switch Output - Pass Front Window - Down
5 | D-GN | -- | Power Window Master Switch Output - Left Rear Window - Up | 5 | D-GN | -- | Power Window Master Switch Output - Left Rear Window - Up
6 | PU | -- | Power Window Master Switch Output - Left Rear Window - Down | 6 | PU | -- | Power Window Master Switch Output - Left Rear Window - Down
7 | BK | -- | Ground | 7 | BK | -- | Ground
8 | L-GN/BK | -- | Power Window Relay Output | 8 | L-GN/BK | -- | Power Window Relay Output
9 | YE (LHD) | -- | Power Mirror Motor Feed - Left Vertical Motor - Up Direction | 9 | YE | -- | Power Mirror Motor Feed - Left Vertical Motor - Up Direction
L-GN (RHD) | --
10 | GY | -- | Power Mirror Motor Feed - Right Horizontal Motor - Left | 10 | GN | -- | Power Mirror Motor Feed - Right Horizontal Motor - Left
11 | L-BU | -- | Power Mirror Motor Feed - Left Horizontal Motor - Left Direction | 11 | L-BU | -- | Power Mirror Motor Feed - Left Horizontal Motor - Left Direction
12 | OG | -- | Heated Mirror Element Feed | 12 | OG | -- | Heated Mirror Element Feed
13 | L-GN | -- | Power Window Master Switch Output - Right Rear Window - Up | 13 | L-GN | -- | Power Window Master Switch Output - Right Rear Window - Up
14 | PU | -- | Power Window Master Switch Output - Right Rear Window - Down | 14 | PU | -- | Power Window Master Switch Output - Right Rear Window - Down
15 | RD/WH | -- | Battery Voltage | 15 | RD/WH | -- | Battery Voltage
16 | BN | -- | Trunk Release Relay Feed-Coil | 16 | BN | -- | Trunk Release Relay Feed-Coil
17 | -- | -- | Not Used | 17 | -- | -- | Not Used
18 | BN/BK | -- | Driver Door Switch Return | 18 | L-GN/RD | -- | Driver Door Switch Return
19 | GY | -- | Speaker Return - Left Front | 19 | GN | -- | Speaker Return - Left Front
20 | BN | -- | Speaker Feed - Left Front | 20 | BN | -- | Speaker Feed - Left Front
21 | WH | -- | HVAC Mode Switch Output | 21 | WH | -- | HVAC Mode Switch Output
22 | RD/BK | -- | Battery Voltage | 22 | RD/BK | -- | Battery Voltage
23 | -- | -- | Not Used | 23 | -- | -- | Not Used
24 | WH | -- | Power Door Lock Relay Feed - Unlock Coil | 24 | WH | -- | Power Door Lock Relay Feed - Unlock Coil
25 | L-BU | -- | Power Door Lock Relay Feed - Lock Coil | 25 | L-BU | -- | Power Door Lock Relay Feed - Lock Coil
26 | BN | -- | Power Door Lock Motor Feed - Unlock | 26 | BN | -- | Power Door Lock Motor Feed - Unlock
27 | GN | -- | Power Door Lock Motor Feed - Lock | 27 | GN | -- | Power Door Lock Motor Feed - Lock
28-29 | -- | -- | Not Used | 28-29 | -- | -- | Not Used

#### C361 Body Harness to Right Front Door Harness

Connector Part Information |

• | MG610692

• | 29-Way F Door (WH)

Connector Part Information

• | MG620693

• | 29-Way M Door Connector (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | D-BU | -- | Power Window Relay Output | 1 | D-BU | -- | Power Window Relay Output
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | L-BU | -- | Power Window Master Switch Output - Pass Front Window - Up | 3 | L-BU | -- | Power Window Master Switch Output - Pass Front Window - Up
4 | BN | -- | Power Window Master Switch Output - Pass Front Window - Down | 4 | PU | -- | Power Window Master Switch Output - Pass Front Window - Down
5-6 | -- | -- | Not Used | 5-6 | -- | -- | Not Used
7 | BK | -- | Ground | 7 | BK | -- | Ground
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | L-GN (LHD) | -- | Power Mirror Motor Feed - Left Vertical Motor - Down Direction | 9 | L-GN | -- | Power Mirror Motor Feed - Left Vertical Motor - Down Direction
YE (RHD) | --
10 | GY | -- | Power Mirror Motor Feed - Right Horizontal Motor - Left Front | 10 | GN | -- | Power Mirror Motor Feed - Right Horizontal Motor - Left Front
11 | WH | -- | Power Mirror Motor Feed - Left Horizontal Motor - Right Direction | 11 | WH | -- | Power Mirror Motor Feed - Left Horizontal Motor - Right Direction
12 | OG | -- | Heated Mirror Element Feed | 12 | OG | -- | Heated Mirror Element Feed
13-17 | -- | -- | Not Used | 13-17 | -- | -- | Not Used
18 | BN/BK | -- | Door Key Lock Cylinder Switch Signal - Passenger | 18 | L-GN/RD | -- | Door Key Lock Cylinder Switch Signal - Passenger
19 | D-GN | -- | Speaker Return - RF | 19 | GY | -- | Speaker Return - RF
20 | L-GN | -- | Speaker Feed - Right Front | 20 | L-GN | -- | Speaker Feed - Right Front
21-25 | -- | -- | Not Used | 21-25 | -- | -- | Not Used
26 | BN | -- | Power Door Lock Motor Feed - Unlock | 26 | BN | -- | Power Door Lock Motor Feed - Unlock
27 | GY | -- | Power Door Lock Motor Feed - Lock | 27 | GY | -- | Power Door Lock Motor Feed - Lock
28 | L-BU | -- | Power Door Lock - Lock | 28 | L-BU | -- | Power Door Lock - Lock
29 | WH | -- | Power Door Lock - Unlock | 29 | WH | -- | Power Door Lock - Unlock

#### C371 Body Harness to Left Rear Door Harness

Connector Part Information |

• | KET MG 651044

• | 6-Way F 090 II Series (WH)

Connector Part Information

• | KET MG 641047

• | 6-Way M 090 II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | GY | -- | Power Door Lock Motor Feed - Lock | 1 | GY | -- | Power Door Lock Motor Feed - Lock
2 | BN | -- | Power Door Lock Motor Feed - Unlock | 2 | BN | -- | Power Door Lock Motor Feed - Unlock
3 | PU | -- | Power Window Master Switch Output - Left Rear Window - Down | 3 | PU | -- | Power Window Master Switch Output - Left Rear Window - Down
4 | D-GN | -- | Power Window Master Switch Output - Left Rear Window - Up | 4 | D-GN | -- | Power Window Master Switch Output - Left Rear Window - Up
5 | D-BU | -- | Power Window Master Switch Output - Lockout | 5 | D-BU | -- | Power Window Master Switch Output - Lockout
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

#### C381 Body Harness to Left Rear Door Harness

Connector Part Information |

• | KET MG 651044

• | 6-Way F 090 II Series (WH)

Connector Part Information

• | KET MG 641047

• | 6-Way M 090 II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | GY | -- | Power Door Lock Motor Feed - Lock | 1 | GY | -- | Power Door Lock Motor Feed - Lock
2 | BN | -- | Power Door Lock Motor Feed - Unlock | 2 | BN | -- | Power Door Lock Motor Feed - Unlock
3 | PU | -- | Power Window Master Switch Output - Right Rear Window - Down | 3 | PU | -- | Power Window Master Switch Output - Right Rear Window - Down
4 | D-GN | -- | Power Window Master Switch Output - Right Rear Window - Up | 4 | D-GN | -- | Power Window Master Switch Output - Right Rear Window - Up
5 | D-BU | -- | Power Window Master Switch Output - Lockout | 5 | D-BU | -- | Power Window Master Switch Output - Lockout
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

#### C401 Floor Harness to Trunk Harness

Connector Part Information |

• | MG610402

• | 8-Way F Series Sealed (WH)

Connector Part Information

• | MG620403

• | 8-Way M Series Sealed (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BN/WH | -- | Park Lamp Feed - Right | 1 | PU | -- | Park Lamp Feed - Right
2 | L-GN | -- | Backup Lamp Feed | 2 | L-GN | -- | Backup Lamp Feed
3 | OG | -- | Fog Lamp Feed - Rear | 3 | OG | -- | Fog Lamp Feed - Rear
4 | PU | -- | Park Lamp Feed - Left | 4 | PU | -- | Park Lamp Feed - Left
5 | L-BU | -- | Turn Signal Lamp Feed - Left Front | 5 | L-BU | -- | Turn Signal Lamp Feed - Left Front
6 | D-BU | -- | Turn Signal Lamp Feed - Right Front | 6 | D-BU | -- | Turn Signal Lamp Feed - Right Front
7 | L-BU | -- | Stop Lamp Feed | 7 | L-BU | -- | Stop Lamp Feed
8 | -- | -- | Not Used | 8 | -- | -- | Not Used

#### C402 Trunk Lid Harness to Floor Harness

Connector Part Information |

• | KET MG 651050

• | 6-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641053

• | 6-Way M 090-II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BN | -- | Trunk Release Relay Feed-Coil | 1 | BN | -- | Trunk Release Relay Feed-Coil
2 | L-BU | -- | Stop Lamp Feed | 2 | L-BU | -- | Stop Lamp Feed
3 | PU | -- | Park Lamp Feed - Left | 3 | PU | -- | Park Lamp Feed - Left
4 | L-BU | -- | Tamper Switch Signal | 4 | L-BU | -- | Tamper Switch Signal
5 | GY/BK | -- | Trunk Lamp Output | 5 | GY/BK | -- | Trunk Lamp Output
6 | BK | -- | Ground | 6 | BK | -- | Ground

#### C415 Rear Harness to Left Tail Lamp Jumper

Connector Part Information |

• | KET MG 610152

• | 6-Way F 090 (2.3 mm) Series (WH)

Connector Part Information

• | KET MG 620153

• | 6-Way M 090 (2.3 mm) Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BK | 450 | Ground | 1 | BK | 450 | Ground
2 | BK | 450 | Ground | 2 | BK/YE | 450 | Ground
3 | L-GN | 24 | Backup Lamp Supply Voltage (w/Backup Lamp) | 3 | WH | 24 | Backup Lamp Supply Voltage
RD | 122 | Rear Fog Lamp Supply Voltage w/Rear Fog Lamp (RHD) | WH | 122 | Rear Fog Lamp Supply Voltage w/Rear Fog Lamp
4 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | 4 | YE | 14 | Left Turn Signal Lamps Supply Voltage
5 | PU | 709 | Left Park Lamp Supply Voltage | 5 | D-BU | 709 | Left Park Lamp Supply Voltage
6 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 6 | RD | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal

#### C416 Rear Harness to Right Tail Lamp Jumper (Notchback)

Connector Part Information |

• | KET MG 610152

• | 6-Way F 090 (2.3 mm) Series (WH)

Connector Part Information

• | KET MG 620153

• | 6-Way M 090 (2.3 mm) Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BK | 450 | Ground | 1 | BK | 450 | Ground
2 | BK | 450 | Ground | 2 | BK/YE | 450 | Ground
3 | L-GN | 24 | Backup Lamp Supply Voltage (w/Backup Lamp) | 3 | WH | 24 | Backup Lamp Supply Voltage
RD | 122 | Rear Fog Lamp Supply Voltage w/Rear Fog Lamp (RHD) | WH | 122 | Rear Fog Lamp Supply Voltage w/Rear Fog Lamp
4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 4 | YE | 15 | Right Turn Signal Lamps Supply Voltage
5 | PU/BK | 309 | Right Park Lamp Supply Voltage | 5 | D-BU | 709 | Right Park Lamp Supply Voltage
6 | YE | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 6 | RD | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal

#### C417 Rear Harness to Marker Lamp Jumper

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (BK)

Connector Part Information

• | KET MG 640322

• | 2-Way SWP Series (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | PU | 709 | Park Lamp Supply Voltage | 1 | BN | 709 | Park Lamp Supply Voltage
2 | BK | 250 | Ground | 2 | BK | 250 | Ground

## Inline Harness Connector End Views Hatchback

Table 1: | C101 TCM Harness to Engine Harness
Table 2: | C102 Front Harness to Engine Harness
Table 3: | C104 Body Harness to Front Harness
Table 4: | C106 Body Harness to Front Harness (RHD)
Table 5: | C107 Body Harness to Front Harness (RHD)
Table 6: | C113 Front Harness to Left Turn Signal Jumper
Table 7: | C114 Front Harness to Right Turn Signal Jumper
Table 8: | C201 Front Harness to I/P Harness (LHD) Body Harness to Front Harness (RHD)
Table 9: | C202 TCM Harness to I/P Harness
Table 10: | C203 Front Harness to I/P Harness (LHD) I/P Harness to Body Harness (RHD)
Table 11: | C204 Front Harness to I/P Harness
Table 12: | C205 Engine Harness to I/P Harness
Table 13: | C210 I/P Harness to Body Harness
Table 14: | C211 Front Harness to Body Harness
Table 15: | C212 I/P Harness to Body Harness
Table 16: | C213 I/P Harness to Body Harness
Table 17: | C214 Air Bag Harness to I/P Harness (except North America)
Table 18: | C214 Air Bag Harness to I/P Harness (North America)
Table 19: | C215 Engine Harness to I/P Harness
Table 20: | C216 Body Harness to Left Rear Door Harness
Table 21: | C351 Body Harness to Driver Door Harness
Table 22: | C361 Body Harness to Passenger Door Harness
Table 23: | C371 Body Harness to Left Rear Door Harness
Table 24: | C381 Body Harness to Right Rear Door Harness
Table 25: | C401 Body Harness to Tailgate Harness
Table 26: | C402 Tailgate Harness to Tailgate Extension Harness
Table 27: | C403 Tailgate Harness to Tailgate Extension Harness
Table 28: | C404 Body Harness to Tailgate Harness
Table 29: | C415 Body Harness to Left Tail Lamp Jumper
Table 30: | C416 Body Harness to Left Tail Lamp Jumper
Table 31: | C417 Rear Harness to Marker Lamp Jumper

#### C101 TCM Harness to Engine Harness

Connector Part Information |

• | AMP 174257-2

• | 4-Way F 070 Series Econoseal-J MK-2 Cap Hsg 4P (BK)

Connector Part Information

• | AMP 174259-2

• | 4-Way M 070 Series Econoseal J MK-2 Plug Ass'y 4P (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BK/WH | 251 | Ground | 1 | BK/WH | 251 | Ground
2 | L-GN | 24 | Backup Lamp Supply Voltage | 2 | L-GN | 24 | Backup Lamp Supply Voltage
3 | YE | 710 | CAN Serial Data Low | 3 | YE | 710 | CAN Serial Data Low
4 | PU | 1807 | CAN Serial Data High | 4 | PU | 1807 | CAN Serial Data High

#### C102 Front Harness to Engine Harness

Connector Part Information |

• | PK 145-20017 (KUM)

• | 20-Way F AR 20F-W Ass'y (WH)

Connector Part Information

• | PK 141-20017 (KUM)

• | 20-Way M AR 20M-W Ass'y (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | L-BU | 1937 | Fuel Level Sensor Low Reference | 1 | L-BU | 1937 | Fuel Level Sensor Low Reference
2 | GY | 1936 | Fuel Level Sensor Signal | 2 | GY | 1936 | Fuel Level Sensor Signal
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | L-GN | 24 | Backup Lamp Supply Voltage | 4 | L-GN/BK | 24 | Backup Lamp Supply Voltage
5 | D-GN | 834 | Rough Road Signal (w/ABS) | 5 | WH | 834 | Rough Road Signal (w/ABS)
6 | GY | 473 | High Speed Cooling Fan Relay Control | 6 | GY | 473 | High Speed Cooling Fan Relay Control
7 | GY | 355 | Low Speed Cooling Fan Relay Control | 7 | D-GN | 355 | Low Speed Cooling Fan Relay Control
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | BN | 1733 | Ignition 1 Voltage | 9 | BN | 1733 | Ignition 1 Voltage
BN | 1733 | Ignition 1 Voltage (MR-140)
10 | D-GN/BK | 1670 | HO2S 2 Low Reference Sensor | 10 | D-GN/BK | 1670 | HO2S 2 Low Reference Sensor
11 | L-GN | 413 | HO2S 2 High Signal Sensor | 11 | L-GN | 413 | HO2S 2 High Signal Sensor
12 | BN | 1671 | HO2S 2 Heater Low Control Sensor | 12 | BN | 1671 | HO2S 2 Heater Low Control Sensor
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | L-BU | 1030 | Low Reference | 14 | L-BU | 1030 | Low Reference
15 | WH/RD | 1031 | 5-Volt Reference | 15 | WH/D-BU | 1031 | 5-Volt Reference
16 | PK | 1733 | Main Relay Output | 16 | PK | 1733 | Main Relay Output
17 | YE/D-BU | 497 | Fuel Pump Relay Control | 17 | YE/BK | 497 | Fuel Pump Relay Control
18 | D-GN | 67 | A/C Compressor Clutch Coil Supply Voltage | 18 | D-GN | 67 | A/C Compressor Clutch Coil Supply Voltage
19-20 | -- | -- | Not Used | 19-20 | -- | -- | Not Used

#### C104 Body Harness to Front Harness

Connector Part Information |

• | KET MG 651068

• | 15-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641071-1

• | 15-Way M 090-II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | GY/D-GN | 711 | Left Headlamp High Beam Supply Voltage | 1 | GY/D-GN | 11 | Left Headlamp High Beam Supply Voltage
2 | WH/BK | 1346 | Headlamp Supply Voltage/Headlamp Control | 2 | WH/BK | 1346 | Headlamp Supply Voltage/Headlamp Control
3 | OG | 140 | Battery Positive Voltage | 3 | -- | -- | Not Used
4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
5 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | 5 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | BN | 1080 | Park Lamp Relay Control | 7 | BN | 1080 | Park Lamp Relay Control
8 | WH | 352 | Headlamp Relay Coil Supply Voltage | 8 | WH | 352 | Headlamp Relay Coil Supply Voltage
9 | YE/GN | 712 | Left Headlamp Low Beam Supply Voltage | 9 | YE/GN | 12 | Left Headlamp Low Beam Supply Voltage
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | D-GN/WH | 94 | Windshield Washer Switch Signal | 11 | D-GN/WH | 94 | Windshield Washer Switch Signal
12 | RD | 441 | Ignition 3 Voltage | 12 | RD | 441 | Ignition 3 Voltage
13 | D-GN | 96 | Windshield Washer Switch Pulse Delay Signal | 13 | D-GN | 96 | Windshield Washer Switch Pulse Delay Signal
14 | D-BU | 92 | Windshield Wiper Motor Low Speed | 14 | D-BU | 92 | Windshield Wiper Motor Low Speed
15 | WH | 95 | Windshield Wiper Motor High Speed | 15 | WH | 95 | Windshield Wiper Motor High Speed

#### C106 Body Harness to Front Harness (RHD)

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (BK)

Connector Part Information

• | KET MG 641053-2

• | 8-Way M 090-II Series (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 1 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
2 | WH/YE | 318 | Front Fog Lamp Supply Voltage | 2 | WH/YE | 318 | Front Fog Lamp Supply Voltage
3 | BK | 28 | Horn Relay Control | 3 | BK | 28 | Horn Relay Control
4 | GN | 189 | Headlamp Leveling Motor Supply Voltage | 4 | GN | 189 | Headlamp Leveling Motor Supply Voltage
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | BN/BK | 109 | Hood Ajar Switch Signal | 6 | BN/BK | 109 | Hood Ajar Switch Signal
7 | PU | 239 | Ignition 1 Voltage | 7 | PU | 239 | Ignition 1 Voltage
8 | -- | -- | Not Used | 8 | -- | -- | Not Used

#### C107 Body Harness to Front Harness (RHD)

Connector Part Information |

• | KET MG 651056

• | 10-Way F 090-II Connector (WH)

Connector Part Information

• | KET MG 641059-5

• | 10-Way M 090-II Connector (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | OG | 1142 | Battery Positive Voltage | 1 | OG/GN | 1142 | Battery Positive Voltage
2 | RD | 242 | Ignition 3 Voltage | 2 | RD | 242 | Ignition 3 Voltage
3 | L-GN | 867 | ABS Indicator Control | 3 | L-GN | 867 | ABS Indicator Control
4 | BK/WH | 2051 | Serial Data | 4 | BK/WH | 2051 | Serial Data
5 | L-GN/BK | 392 | Rear Window Washer Pump Control | 5 | L-GN/BK | 392 | Rear Window Washer Pump Control
6 | BN | 33 | Brake Warning Indicator Control | 6 | BN | 33 | Brake Warning Indicator Control
7 | PK | 639 | Ignition 3 Voltage (Mando ABS) | 7 | PK | 639 | Ignition 3 Voltage (Mando ABS)
8 | BN | 1541 | Ignition 1 Voltage | 8 | BN | 1541 | Ignition 1 Voltage
9 | BN/WH | 309 | Right Park Lamp Supply Voltage | 9 | BN/WH | 309 | Right Park Lamp Supply Voltage
10 | -- | -- | Not Used | 10 | -- | -- | Not Used

#### C113 Front Harness to Left Turn Signal Jumper

Connector Part Information |

• | KET MG 641234

• | 3-Way F SSD & 0509 (BK)

Connector Part Information

• | KET MG 611611

• | 3-Way M SSD & 0509 Connector (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | BN | 709 | Left Park Lamp Supply Voltage
2 | BK | 50 | Ground | 2 | BK | 50 | Ground
3 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | 3 | YE | 14 | Left Turn Signal Lamp Supply Voltage

#### C114 Front Harness to Right Turn Signal Jumper

Connector Part Information |

• | KET MG 641234

• | 3-Way F SSD & 0509 (BK)

Connector Part Information

• | KET MG 611611

• | 3-Way M SSD & 0509 Connector (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BN/WH | 309 | Right Park Lamp Supply Voltage | 1 | BN | 709 | Right Park Lamp Supply Voltage
2 | BK | 250 | Ground | 2 | BK | 50 | Ground
3 | D/BU | 15 | Right Turn Signal Lamp Supply Voltage | 3 | YE | 14 | Right Turn Signal Lamp Supply Voltage

#### C201 Front Harness to I/P Harness (LHD) Body Harness to Front Harness (RHD)

Connector Part Information |

• | KET MG 651074-2

• | 18-Way F 090-II Connector (BU)

Connector Part Information

• | KET MG 641077-2

• | 18-Way M 090-II Connector (BU)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | OG/D-GN | 1142 | Battery Positive Voltage | 1 | OG/D-GN | 1142 | Battery Positive Voltage
2 | RD | 242 | Ignition 1 Voltage | 2 | RD | 242 | Ignition 1 Voltage
3 | L-GN | 867 | ABS Indicator Control | 3 | L-GN | 867 | ABS Indicator Control
4 | BK/WH | 2051 | Serial Data (w/ABS) | 4 | BK/WH | 2051 | Serial Data (w/ABS)
5 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal (w/ABS) | 5 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal (w/ABS)
6 | WH/YE | 318 | Front Fog Lamp Supply Voltage | 6 | WH/YE | 318 | Front Fog Lamp Supply Voltage
7 | BK | 28 | Horn Relay Control (w/SIR) | 7 | BK | 28 | Horn Relay Control (w/SIR)
BK/WH | 29 | Horn Control (w/o SIR) | BK/WH | 29 | Horn Control (w/o SIR)
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | L-GN/BK | 392 | Rear Window Washer Pump Control (w/Rear Window Washer) | 9 | L-GN/BK | 392 | Rear Window Washer Pump Control (w/Rear Window Washer)
10 | BN | 33 | Brake Warning Indicator Control | 10 | BN | 33 | Brake Warning Indicator Control
BN/WH | 133 | Brake Warning Indicator Control (LHD) | BN/WH | 133 | Brake Warning Indicator Control (LHD)
11 | PK | 639 | Ignition 1 Voltage (Mando ABS) | 11 | PK | 639 | Ignition 1 Voltage (Mando ABS)
12 | BN | 1541 | Ignition 1 Voltage | 12 | BN | 1541 | Ignition 1 Voltage
13 | BN/WH | 309 | Right Park Lamp Supply Voltage | 13 | BN/WH | 309 | Right Park Lamp Supply Voltage
14 | L-BU | 1769 | Fog Lamp Indicator Control (w/Fog Lamps) | 14 | L-BU | 1769 | Fog Lamp Indicator Control
15 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage (Except North America) | 15 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage (Except North America)
16 | PU | 172 | Low Fuel Indicator Control (LHD) | 16 | PU | 172 | Low Fuel Indicator Control (LHD)
17 | BN/BK | 109 | Hood Ajar Switch Signal | 17 | BN/BK | 109 | Hood Ajar Switch Signal
18 | PK | 239 | Ignition 1 Voltage (HV-240) | 18 | PK | 239 | Ignition 1 Voltage

#### C202 TCM Harness to I/P Harness

Connector Part Information |

• | KET MG 651350

• | 11-Way F 090-II (WH)

Connector Part Information

• | KET MG 641353

• | 11-Way M 090-II (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BN | 323 | Park/Neutral Position (PNP) Switch Park Signal | 1 | BN | 323 | Park/Neutral Position (PNP) Switch Park Signal
2-3 | -- | -- | Not Used | 2-3 | -- | -- | Not Used
4 | D-GN/WH | 1135 | Hold Mode Signal | 4 | D-GN/WH | 1135 | Hold Mode Signal
5 | YE | 1481 | Hold Mode Indicator Control | 5 | YE | 1481 | Hold Mode Indicator Control
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 7 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
8 | D-BU | 2051 | Serial Data | 8 | BK/WH | 2051 | Serial Data
9 | D-GN/WH | 817 | Vehicle Speed Signal | 9 | D-GN/WH | 817 | Vehicle Speed Signal
D-GN/WH | 817 | Vehicle Speed Signal
10 | PK | 839 | Ignition 1 Voltage | 10 | PK | 839 | Ignition 1 Voltage
11 | OG | 440 | Battery Positive Voltage | 11 | OG | 440 | Battery Positive Voltage

#### C203 Front Harness to I/P Harness (LHD) I/P Harness to Body Harness (RHD)

Connector Part Information |

• | KET MG 651110-5

• | 14-Way F 090-II Series (BK)

Connector Part Information

• | KET MG 641113-5

• | 14-Way M 090-II Series (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | OG | 140 | Battery Positive Voltage | 1 | OG | 140 | Battery Positive Voltage
2 | WH/BK | 1346 | Headlamp Supply Voltage/Headlamp Control | 2 | WH/BK | 1346 | Headlamp Supply Voltage/Headlamp Control
3 | GY/D-GN | 11 | Headlamp High Beam Supply Voltage | 3 | GY/D-GN | 11 | Headlamp High Beam Supply Voltage
4 | YE/D-GN | 12 | Headlamp Low Beam Supply Voltage | 4 | YE/D-GN | 12 | Headlamp Low Beam Supply Voltage
5 | WH | 352 | Headlamp Relay Coil Supply Voltage | 5 | WH | 352 | Headlamp Relay Coil Supply Voltage
6 | BN | 1080 | Park Lamp Relay Control | 6 | BN | 1080 | Park Lamp Relay Control
7 | PU | 293 | Rear Defog Element Supply Voltage | 7 | PU | 293 | Rear Defog Element Supply Voltage
8 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | 8 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
9 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage | 9 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
10 | WH | 95 | Windshield Wiper Motor High Speed | 10 | WH | 95 | Windshield Wiper Motor High Speed
11 | D-BU | 92 | Windshield Wiper Motor Low Speed | 11 | D-BU | 92 | Windshield Wiper Motor Low Speed
12 | D-GN | 96 | Windshield Wiper Switch Pulse Delay Signal | 12 | D-GN | 96 | Windshield Wiper Switch Pulse Delay Signal
13 | RD | 441 | Ignition 3 Voltage | 13 | RD | 441 | Ignition 3 Voltage
14 | D-GN/WH | 94 | Windshield Washer Switch Signal | 14 | D-GN/WH | 94 | Windshield Washer Switch Signal

#### C204 Front Harness to I/P Harness

Connector Part Information |

• | KET MG 651926

• | 4-Way F 312-II Series (WH)

Connector Part Information

• | KET MG 641928

• | 4-Way M 312-II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | OG/BK | 142 | Battery Positive Voltage | 1 | OG | 142 | Battery Positive Voltage
2 | RD/BK | 141 | Ignition 3 Voltage | 2 | RD/BK | 141 | Ignition 3 Voltage
3 | YE | 143 | Accessory Voltage | 3 | YE | 143 | Accessory Voltage
4 | RD/BK | 141 | Ignition 3 Voltage | 4 | RD/BK | 141 | Ignition 3 Voltage

#### C205 Engine Harness to I/P Harness

Connector Part Information |

• | KET MG 611810-41

• | 18-Way F Device Connector (GY)

Connector Part Information

• | KET MG 652426

• | 36-Way M Door 36P Hsg (090-II) (GY)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | YE | 5 | Crank Voltage (Except Auto Transmission North America) | 1 | YE | 5 | Crank Voltage (Except Auto Transmission North America)
PU | 6 | Starter Solenoid Crank Voltage (Automatic Transmission North America) | 1 | PU | 6 | Starter Solenoid Crank Voltage (Automatic Transmission North America)
2 | PK | 539 | Ignition 1 Voltage | 2 | PK | 539 | Ignition 1 Voltage
3 | WH | 30 | Fuel Level Sensor Signal | 3 | WH | 30 | Fuel Level Sensor Signal
4 | D-BU | 2051 | Serial Data (w/Immobilizer) | 4 | BK/WH | 2051 | Serial Data
BK/WH | 2051 | Serial Data (w/o Immobilizer)
5 | YE | 1578 | EVAP Canister Vent Solenoid Control (North America) | 5 | YE | 1578 | EVAP Canister Vent Solenoid Control (North America)
6 | WH | 135 | ECT Sensor Gage Signal | 6 | WH | 135 | ECT Sensor Gage Signal
7 | D-BU | 25 | Charge Indicator Control/Charge Indicator Signal | 7 | D-BU | 25 | Charge Indicator Control/Charge Indicator Signal
8 | PK | 839 | Ignition 1 Voltage | 8 | PK | 839 | Ignition 1 Voltage
1739 | 1739
9 | D-GN/WH | 762 | A/C Request Signal | 9 | D-GN/WH | 762 | A/C Request Signal
10 | BN | 732 | Evaporator Temperature Sensor Signal (1.2L) | 10 | BN | 732 | Evaporator Temperature Sensor Signal
11 | OG | 440 | Battery Positive Voltage | 11 | OG | 440 | Battery Positive Voltage
12 | L-BU | 733 | Reference Low (1.4L) | 12 | L-BU | 733 | Reference Low (1.4L)
BN | Reference Low (1.2L) | BN | Reference Low (1.2L)
13 | PK/D-BU | 439 | Ignition 1 Voltage (w/Manual Transmission) | 13 | PK | 439 | Ignition 1 Voltage (w/Manual Transmission)
14 | D-GN/WH | 817 | Vehicle Speed Signal (w/Manual Transmission) | 14 | D-GN/WH | 817 | Vehicle Speed Signal
15 | WH | 121 | Engine Speed Signal | 15 | WH | 121 | Engine Speed Signal
16 | BN/BK | 419 | MIL Control | 16 | BN/BK | 419 | Malfunction Indicator Lamp (MIL) Control
17 | D-GN | 31 | Oil Pressure Indicator Control | 17 | D-GN/WH | 31 | Oil Pressure Indicator Control
18 | PU/WH | 821 | Engine Overspeed Indicator Control (w/Overspeed Warning) | 18 | BN/BK | 821 | Engine Overspeed Indicator Control

#### C210 I/P Harness to Body Harness

Connector Part Information |

• | KET MG 651050-2

• | 8-Way F 090-II Series (BU)

Connector Part Information

• | KET MG 641053

• | 8-Way M 090-II Series (BU)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | YE | 749 | Security Indicator Control | 1 | YE | 749 | Security Indicator Control
2 | BK/WH | 2051 | Serial Data | 2 | BK/WH | 2051 | Serial Data
3 | PK | 239 | Ignition 1 Voltage | 3 | PK | 239 | Ignition 1 Voltage
4 | RD/WH | 740 | Battery Positive Voltage (LHD) | 4 | RD/WH | 740 | Battery Positive Voltage (LHD)
5 | YE | 1578 | EVAP Canister Vent Solenoid Control | 5 | YE | 1578 | EVAP Canister Vent Solenoid Control
6 | L-GN | 80 | Key in Ignition Switch Signal | 6 | L-GN | 80 | Key in Ignition Switch Signal
7 | BN/BK | 109 | Hood Ajar Switch Signal | 7 | BN/BK | 109 | Hood Ajar Switch Signal
8 | -- | -- | Not Used | 8 | -- | -- | Not Used

#### C211 Front Harness to Body Harness

Connector Part Information |

• | KET MG 651086-3

• | 22-Way F 090-II Series (YE)

Connector Part Information

• | KET MG 641089-3

• | 22-Way F 090-II Series (YE)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BN/BK | 885 | Left Rear Wheel Speed Sensor Low Reference (w/ABS) | 1 | BN/BK | 885 | Left Rear Wheel Speed Sensor Low Reference
2 | D-GN/WH | 884 | Left Rear Wheel Speed Sensor Signal (w/ABS) | 2 | D-GN/WH | 884 | Left Rear Wheel Speed Sensor Signal
3 | PU | 883 | Right Rear Wheel Speed Sensor Low Reference (w/ABS) | 3 | PU | 883 | Right Rear Wheel Speed Sensor Low Reference
4 | L-BU | 882 | Right Rear Wheel Speed Sensor Signal (w/ABS) | 4 | L-BU | 882 | Right Rear Wheel Speed Sensor Signal
5 | L-GN | 24 | Backup Lamp Supply Voltage | 5 | L-GN | 24 | Backup Lamp Supply Voltage
6 | L-BU | 1937 | Fuel Level Sensor Low Reference | 6 | L-BU | 1937 | Fuel Level Sensor Low Reference
GY/D-GN | 1029 | GY/D-GN | 1029
7 | PU | 709 | Left Park Lamp Supply Voltage | 7 | PU | 709 | Left Park Lamp Supply Voltage
8 | BN/WH | 309 | Right Park Lamp Supply Voltage | 8 | BN/WH | 309 | Right Park Lamp Supply Voltage
9 | BN | 1733 | Ignition 1 Voltage (MR-140) | 9 | BN | 1733 | Ignition 1 Voltage (MR-140)
10 | OG/BK | 540 | Battery Positive Voltage | 10 | BN | 541 | Battery Positive Voltage
11 | PU | 267 | Heated Mirror Element Supply Voltage (LHD) | 11 | PU | 267 | Heated Mirror Element Supply Voltage (Hatchback)
OG | 293 | Heated Mirror Element Supply Voltage (Notchback) | OG | 293 | Heated Mirror Element Supply Voltage (Notchback)
12 | PU | 172 | Low Fuel Indicator Control (LHD) | 12 | PU | 172 | Low Fuel Indicator Control (LHD)
13 | L-GN/BK | 392 | Low Reference | 13 | L-GN/BK | 392 | Low Reference
14 | L-BU | 1030 | Low Reference (MR-140) | 14 | L-BU | 1030 | Low Reference (MR-140)
15 | WH/BU | 1031 | 5-Volt Reference (MR-140) | 15 | WH | 1031 | 5-Volt Reference (MR-140)
16 | L-BU | 1723 | Fuel Pump Supply Voltage | 16 | BN | 1723 | Fuel Pump Supply Voltage
17 | -- | -- | Not Used | 17 | -- | -- | Not Used
18 | BN | 41 | Ignition 3 Voltage (w/Power Windows) | 18 | RD/WH | 41 | Ignition 3 Voltage
19 | GY | 1936 | Fuel Level Sensor Signal | 19 | GY | 1936 | Fuel Level Sensor Signal
20 | -- | -- | Not Used | 20 | -- | -- | Not Used
21 | D-GN/WH | 261 | Arm Alarm Signal | 21 | D-GN/WH | 261 | Arm Alarm Signal
22 | BN | 741 | Ignition 1 Voltage | 22 | BN | 741 | Ignition 1 Voltage

#### C212 I/P Harness to Body Harness

Connector Part Information |

• | KET MG 651056-5

• | 10-Way F 090-II Series (BK)

Connector Part Information

• | KET MG 641059-5

• | 10-Way M 090-II Connector (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | OG | 1340 | Battery Positive Voltage | 1 | OG | 1340 | Battery Positive Voltage
2-3 | -- | -- | Not Used | 2-3 | -- | -- | Not Used
4 | D-GN/WH | 157 | Courtesy Lamp Control | 4 | D-GN/WH | 157 | Courtesy Lamp Control
5 | RD | 441 | Ignition 3 Voltage | 5 | RD | 441 | Ignition 3 Voltage
6 | GY | 393 | Rear Window Wiper Motor Control | 6 | GY | 393 | Rear Window Wiper Motor Control
7 | RD | 122 | Rear Fog Lamp Supply Voltage (Rear Fog Lamps) | 7 | RD | 122 | Rear Fog Lamp Supply Voltage (Rear Fog Lamps)
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | BK/WH | 238 | Seat Belt Switch - Driver | 9 | BK/WH | 238 | Seat Belt Switch - Driver
10 | PU | 126 | Left Front Door Open Switch Signal | 10 | PU | 126 | Left Front Door Open Switch Signal

#### C213 I/P Harness to Body Harness

Connector Part Information |

• | MG651068

• | 15-Way F 090-II Series (WH)

Connector Part Information

• | MG641071

• | 15-Way M 090-II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | OG | 40 | Battery Positive Voltage | 1 | OG | 40 | Battery Positive Voltage
OG | 40 | Battery Positive Voltage (w/Power Mirrors)
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | PU | 172 | Low Fuel Indicator Lamp (RHD) | 3 | PU | 172 | Low Fuel Indicator Lamp (RHD)
4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
D-BU | 15 | Right Turn Signal Lamps Supply Voltage (w/Remote Keyless Entry)
5 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | 5 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
L-BU | 14 | Left Turn Signal Lamp Supply Voltage (w/Remote Keyless Entry)
6 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 6 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
7 | PU | 201 | Left Front Speaker Output (+) | 7 | PU | 201 | Left Front Speaker Output (+)
8 | L-GN | 118 | Left Front Speaker Output (-) | 8 | L-GN | 118 | Left Front Speaker Output (-)
9 | L-BU | 200 | Right Front Speaker Output (+) | 9 | L-BU | 200 | Right Front Speaker Output (+)
10 | BN | 117 | Right Front Speaker Output (-) | 10 | BN | 117 | Right Front Speaker Output (-)
11 | GY | 199 | Left Rear Speaker Output (+) | 11 | GY | 199 | Left Rear Speaker Output (+)
12 | D-GN | 116 | Left Rear Speaker Output (-) | 12 | D-GN | 116 | Left Rear Speaker Output (-)
13 | D-BU | 46 | Right Rear Speaker Output (+) | 13 | D-BU | 46 | Right Rear Speaker Output (+)
14 | WH | 115 | Right Rear Speaker Output (-) | 14 | WH | 115 | Right Rear Speaker Output (-)
15 | BN | 33 | Brake Warning Indicator Control | 15 | BN | 33 | Brake Warning Indicator Control

#### C214 Air Bag Harness to I/P Harness (except North America)

Connector Part Information |

• | MG610396

• | 4-Way F Series Sealed (WH)

Connector Part Information

• | MG620397

• | 4-Way M Series Sealed (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | D-GN/WH | 358 | Air Bag Indicator Control | 1 | D-GN/WH | 358 | Air Bag Indicator Control
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | PK | 139 | Ignition 1 Voltage | 3 | PK | 139 | Ignition 1 Voltage
4 | BN | 337 | SIR Serial Data | 4 | BN | 337 | SIR Serial Data

#### C214 Air Bag Harness to I/P Harness (North America)

Connector Part Information |

• | MG610404

• | 10-Way F 090-II Series (YE)

Connector Part Information

• | MG620405

• | 10-Way M 090-II Connector (YE)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | D-GN/WH | 6169 | Front Discriminating Sensor - LH Signal | 1 | D-GN/WH | 6169 | Front Discriminating Sensor - LH Signal
2 | PU | 1358 | DIC Switch Signal | 2 | PU | 1358 | DIC Switch Signal
3 | L-GN | 6777 | Front Discriminating Sensor - RH Signal | 3 | L-GN | 6777 | Front Discriminating Sensor - RH Signal
4 | PK | 739 | Ignition 1 Voltage | 4 | PK | 739 | Ignition 1 Voltage
5 | YE | 6168 | Front Discriminating Sensor - LH Signal | 5 | YE | 6168 | Front Discriminating Sensor - LH Signal
6 | D-GN/WH | 358 | AIR BAG Indicator Control | 6 | D-GN/WH | 358 | AIR BAG Indicator Control
7 | PK | 139 | Ignition 1 Voltage | 7 | PK | 139 | Ignition 1 Voltage
8 | BN | 337 | Serial Data | 8 | BN | 337 | Serial Data
9 | BN/WH | 6776 | Front Discriminating Sensor - RH Signal | 9 | BN/WH | 6776 | Front Discriminating Sensor - RH Signal
10 | -- | -- | Not Used | 10 | -- | -- | Not Used

#### C215 Engine Harness to I/P Harness

Connector Part Information |

• | KET MG 611810-41

• | 18-Way F Device Connector (GY)

Connector Part Information

• | KET MG 652426

• | 36-Way M Door 36P Hsg (090-II) (GY)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | YE/BK | 183 | Cruise Control Indicator Signal | 1 | YE/BK | 183 | Cruise Control Indicator Signal
2 | L-GN/BU | 474 | 5-Volt Reference | 2 | L-GN | 474 | 5-Volt Reference
3-5 | -- | -- | Not Used | 3-5 | -- | -- | Not Used
6 | D-GN/WH | 397 | Cruise Control ON Switch Output | 6 | D-GN/WH | 397 | Cruise Control ON Switch Output
7 | D-GN/WH | 718 | Accelerator Pedal Sensor Signal Return | 7 | D-GN/WH | 718 | Accelerator Pedal Sensor Signal Return
8 | D-BU | 1161 | Electronic Throttle-Pedal Position Signal 1 | 8 | D-BU | 1161 | Electronic Throttle-Pedal Position Signal 1
9 | GY/BK | 596 | 5-Volt Reference | 9 | GY | 596 | 5-Volt Reference
10 | L-BU | 645 | Accelerator Pedal Sensor Signal Return | 10 | L-BU | 645 | Accelerator Pedal Sensor Signal Return
11 | WH | 1162 | Electronic Throttle-Pedal Position Signal 2 | 11 | WH | 1162 | Electronic Throttle-Pedal Position Signal 2
12 | GY | 474 | 5-Volt Reference | 12 | GY | 474 | 5-Volt Reference
13-18 | -- | -- | Not Used | 13-18 | -- | -- | Not Used

#### C216 Body Harness to Left Rear Door Harness

Connector Part Information |

• | KET MG 651044

• | 6-Way F 090 II Series (WH)

Connector Part Information

• | KET MG 641047

• | 6-Way M 090 II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | BN/WH | 6776 | SIR Inflator Feed - Right Side | 3 | BN/WH | 6776 | SIR Inflator Feed - Right Side
4 | L-GN | 6777 | SIR Inflator Output - Right Side | 4 | L-GN | 6777 | SIR Inflator Output - Right Side
5 | YE | 6168 | SIR Inflator Feed - Left Side | 5 | YE | 6168 | SIR Inflator Feed - Left Side
6 | GY/WH | 6169 | SIR Inflator Output - Left Side | 6 | GY/WH | 6169 | SIR Inflator Output - Left Side

#### C351 Body Harness to Driver Door Harness

Connector Part Information |

• | KET MG 610692

• | 29-Way F Door (WH)

Connector Part Information

• | KET MG 620693

• | 29-Way M Door Connector (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | RD/WH | 41 | Ignition 3 Voltage | 1 | RD/WH | 41 | Ignition 3 Voltage
2 | BN/OG | 1307 | Power Window Master Switch Lockout Control | 2 | BN/OG | 1307 | Power Window Master Switch Lockout Control
3 | D-GN | 166 | Power Window Master Switch Passenger Front Up Signal | 3 | D-GN | 166 | Power Window Master Switch Passenger Front Up Signal
4 | BN | 167 | Power Window Master Switch Passenger Front Down Signal | 4 | BN | 167 | Power Window Master Switch Passenger Front Down Signal
5 | L-GN/RD | 668 | Power Window Motor Left Rear Up Control | 5 | L-GN/RD | 668 | Power Window Motor Left Rear Up Control
6 | GY/D-GN | 169 | Power Window Master Switch Left Rear Down Signal | 6 | GY/D-GN | 169 | Power Window Master Switch Left Rear Down Signal
7 | BK | 650 | Ground | 7 | BK | 650 | Ground
8 | WH | 81 | Mirror Motor Right Control | 8 | WH | 81 | Mirror Motor Right Control
9 | L-GN | 89 | Mirror Motor Up/Down Control | 9 | L-GN | 89 | Mirror Motor Down Control
10 | GY | 90 | Mirror Motor Left Control | 10 | GY | 90 | Mirror Motor Left Control
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | OG | 267 | Heated Mirror Element Supply Voltage | 12 | OG | 267 | Heated Mirror Element Supply Voltage
13 | L-BU | 170 | Power Window Master Switch Right Rear Up Signal | 13 | L-BU | 170 | Power Window Master Switch Right Rear Up Signal
14 | PU | 171 | Power Window Master Switch Right Rear Down Signal | 14 | PU | 171 | Power Window Master Switch Right Rear Down Signal
15-17 | -- | -- | Not Used | 15-17 | -- | -- | Not Used
18 | D-BU | 49 | Door Latch Switch Signal | 18 | PU/D-BU | 49 | Door Latch Switch Signal
19 | L-GN | 118 | Left Front Speaker Output (-) (LHD) | 19 | L-GN | 118 | Left Front Speaker Output (-) (LHD)
BN | 117 | Right Front Speaker Output (-) (RHD) | BN | 117 | Right Front Speaker Output (-) (RHD)
20 | PU | 201 | Left Front Speaker Output (+) (LHD) | 20 | PU | 201 | Left Front Speaker Output (+) (LHD)
L-BU | 200 | Left Front Speaker Output (+) (RHD) | L-BU | 200 | Left Front Speaker Output (+) (RHD)
21-23 | -- | -- | Not Used | 21-23 | -- | -- | Not Used
24 | L-GN | 194 | Door Unlock Control (w/o Dimming) | 24 | L-GN | 194 | Door Unlock Control (w/o Dimming)
25 | GY | 195 | Door Lock Control | 25 | GY | 195 | Door Lock Control
26 | D-BU | 294 | Door Lock Actuator Unlock Control | 26 | D-BU | 294 | Door Lock Actuator Unlock Control
27 | WH | 295 | Door Lock Actuator Lock Control | 27 | WH | 295 | Door Lock Actuator Lock Control
28 | -- | -- | Not Used | 28 | -- | -- | Not Used
29 | OG | 40 | Battery Positive Voltage | 29 | OG | 40 | Battery Positive Voltage

#### C361 Body Harness to Passenger Door Harness

Connector Part Information |

• | KET MG 610692

• | 29-Way F Door (WH)

Connector Part Information

• | KET MG 620693

• | 29-Way M Door Connector (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | BN/OG | 1307 | Power Window Master Switch Lockout Control | 2 | BN/OG | 1307 | Power Window Master Switch Lockout Control
RD/WH | 41 | RD/WH | 41
3 | D-GN | 166 | Power Window Master Switch Passenger Front Up Signal | 3 | D-GN | 166 | Power Window Master Switch Passenger Front Up Signal
4 | BN | 167 | Power Window Master Switch Passenger Front Down Signal | 4 | BN | 167 | Power Window Master Switch Passenger Front Down Signal
5-6 | -- | -- | Not Used | 5-6 | -- | -- | Not Used
7 | BK | 150 | Ground | 7 | BK | 150 | Ground
8 | WH | 81 | Mirror Motor Right Control | 8 | WH | 81 | Mirror Motor Right Control
9 | L-GN | 89 | Mirror Motor Up/Down Control | 9 | L-GN | 89 | Mirror Motor Up/Down Control
10 | GY | 90 | Mirror Motor Left Control | 10 | GY | 90 | Mirror Motor Left Control
11 | BK | 1150 | Ground | 11 | BK | 1150 | Ground
12 | OG | 267 | Heater Mirror Element Supply Voltage | 12 | OG | 267 | Heater Mirror Element Supply Voltage
13-17 | -- | -- | Not Used | 13-17 | -- | -- | Not Used
18 | D-BU | 49 | Door Latch Switch Signal | 18 | D-BU | 49 | Door Latch Switch Signal
19 | BN | 117 | Right Front Speaker Output (-) | 19 | BN | 117 | Right Front Speaker Output (-)
L-GN | 118 | Left Front Speaker Output (-) (RHD) | L-GN | 118 | Left Front Speaker Output (-) (RHD)
20 | L-BU | 200 | Right Front Speaker Output (+) | 20 | L-BU | 200 | Right Front Speaker Output (+)
PU | 201 | Left Front Speaker Output (+) (RHD) | PU | 201 | Left Front Speaker Output (+) (RHD)
21-25 | -- | -- | Not Used | 21-25 | -- | -- | Not Used
26 | D-BU | 294 | Door Lock Actuator Unlock Control | 26 | D-BU | 294 | Door Lock Actuator Unlock Control
27 | WH | 295 | Door Lock Actuator Lock Control | 27 | WH | 295 | Door Lock Actuator Lock Control
28-29 | -- | -- | Not Used | 28-29 | -- | -- | Not Used

#### C371 Body Harness to Left Rear Door Harness

Connector Part Information |

• | KET MG 651044

• | 6-Way F 090 II Series (WH)

Connector Part Information

• | KET MG 641047

• | 6-Way M 090 II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | WH | 295 | Door Lock Actuator Lock Control | 1 | WH | 295 | Door Lock Actuator Lock Control
2 | D-BU | 294 | Door Lock Actuator Unlock Control | 2 | D-BU | 294 | Door Lock Actuator Unlock Control
3 | GY/D-GN | 169 | Power Window Master Switch Left Rear Down Signal | 3 | GY/RD | 169 | Power Window Master Switch Left Rear Down Signal
4 | L-GN/RD | 668 | Power Window Motor Left Rear Up Control | 4 | L-GN/BK | 168 | Power Window Motor Left Rear Up Control
5 | BN/OG | 1307 | Power Window Master Switch Lockout Control | 5 | BN/OG | 1307 | Power Window Master Switch Lockout Control
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

#### C381 Body Harness to Right Rear Door Harness

Connector Part Information |

• | KET MG 651044

• | 6-Way F 090 II Series (WH)

Connector Part Information

• | KET MG 641047

• | 6-Way M 090 II Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | WH | 295 | Door Lock Actuator Lock Control | 1 | WH | 295 | Door Lock Actuator Lock Control
2 | D-BU | 294 | Door Lock Actuator Unlock Control | 2 | D-BU | 294 | Door Lock Actuator Unlock Control
3 | PU | 171 | Power Window Master Switch Left Rear Down Signal | 3 | GY/OG | 169 | Power Window Master Switch Right Rear Down Signal
4 | L-BU | 170 | Power Window Master Switch Right Rear Up Signal | 4 | L-GN/BK | 168 | Power Window Master Switch Right Rear Up Signal
5 | BN/OG | 1307 | Power Window Master Switch Lockout Control | 5 | BN/OG | 1307 | Power Window Master Switch Lockout Control
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

#### C401 Body Harness to Tailgate Harness

Connector Part Information |

• | MG610402

• | 8-Way F Series Sealed (WH)

Connector Part Information

• | MG620403

• | 8-Way M Series Sealed (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | PU | 709 | Left Park Lamp Supply Voltage
2 | BK | 293 | Rear Defog Element Supply Voltage | 2 | BK | 293 | Rear Defog Element Supply Voltage
3 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 3 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
4 | RD | 441 | Ignition 3 Voltage | 4 | RD | 441 | Ignition 3 Voltage
5 | GY | 393 | Rear Window Wiper Motor Control | 5 | GY | 393 | Rear Window Wiper Motor Control
6 | OG/BK | 737 | Rear Compartment Lid Ajar Switch Signal | 6 | OG/BK | 737 | Rear Compartment Lid Ajar Switch Signal
7 | D-BU | 49 | Tamper Switch Signal | 7 | D-BU | 49 | Tamper Switch Signal
8 | BK | 850 | Ground | 8 | BK | 850 | Ground

#### C402 Tailgate Harness to Tailgate Extension Harness

Connector Part Information |

• | KET MG 630680

• | 4-Way 090-II M Series (WH)

Connector Part Information

• | KET MG 620160

• | 4-Way M 090 (2.3 mm) Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | PU | 709 | Left Park Lamp Supply Voltage
2 | OG/BK | 737 | Rear Compartment Lid Ajar Switch Signal | 2 | OG/BK | 737 | Rear Compartment Lid Ajar Switch Signal
3 | BK | 850 | Ground | 3 | BK | 850 | Ground
4 | D-BU | 49 | Tamper Switch Signal | 4 | D-BU | 49 | Tamper Switch Signal

#### C403 Tailgate Harness to Tailgate Extension Harness

Connector Part Information |

• | KET MG 620395

• | 3-Way F 090 (2.3 MM) Series (WH)

Connector Part Information

• | KET MG 610394

• | 3-Way M 090 (2.3 MM) Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | GY | 393 | Rear Window Wiper Motor Control | 1 | GY | 393 | Rear Window Wiper Motor Control
2 | RD | 441 | Ignition 3 Voltage | 2 | RD | 441 | Ignition 3 Voltage
3 | L-GN/BK | 392 | Not Used | 3 | -- | -- | Not Used

#### C404 Body Harness to Tailgate Harness

Connector Part Information |

• | KET MG 610489

• | 2-Way F 090 (2.3 mm) Series (WH)

Connector Part Information

• | KET MG 620490

• | 2-Way M 090 (2.3 mm) Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | D-BU | 294 | Door Lock Actuator Unlock Control | 1 | D-BU | 294 | Door Lock Actuator Unlock Control
2 | WH | 295 | Door Lock Actuator Lock Control | 2 | WH | 295 | Door Lock Actuator Lock Control

#### C415 Body Harness to Left Tail Lamp Jumper

Connector Part Information |

• | KET MG 610152

• | 6-Way F 090 (2.3 mm) Series (WH)

Connector Part Information

• | KET MG 620153

• | 6-Way M 090 (2.3 mm) Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BK | 850 | Ground | 1 | BK | 450 | Ground
2 | BK | 850 | Ground | 2 | BK/YE | 450 | Ground
3 | L-GN | 24 | Backup Lamp Supply Voltage (w/Backup Lamp) | 3 | WH | 24 | Backup Lamp Supply Voltage
4 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | 4 | YE | 14 | Left Turn Signal Lamps Supply Voltage
5 | PU | 709 | Left Park Lamp Supply Voltage | 5 | D-BU | 709 | Left Park Lamp Supply Voltage
PU | 709 | Left Park Lamp Supply Voltage | D-BU | 709 | Left Park Lamp Supply Voltage
6 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 6 | RD | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal

#### C416 Body Harness to Left Tail Lamp Jumper

Connector Part Information |

• | KET MG 610152

• | 6-Way F 090 (2.3 mm) Series (WH)

Connector Part Information

• | KET MG 620153

• | 6-Way M 090 (2.3 mm) Series (WH)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | BK | 950 | Ground | 1 | BK | 450 | Ground
2 | BK | 950 | Ground | 2 | BK/YE | 450 | Ground
3 | L-GN | 24 | Backup Lamp Supply Voltage (w/Backup Lamp) | 3 | WH | 24 | Backup Lamp Supply Voltage
RD | 122 | Rear Fog Lamp Supply Voltage w/Rear Fog Lamp (RHD) | WH | 122 | Rear Fog Lamp Supply Voltage w/Rear Fog Lamp
4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 4 | YE | 15 | Right Turn Signal Lamps Supply Voltage
5 | BN/WH | 309 | Right Park Lamp Supply Voltage | 5 | D-BU | 709 | Right Park Lamp Supply Voltage
6 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 6 | RD | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal

#### C417 Rear Harness to Marker Lamp Jumper

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (BK)

Connector Part Information

• | KET MG 640322

• | 2-Way SWP Series (BK)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
1 | PU | 709 | Park Lamp Supply Voltage | 1 | BN | 709 | Park Lamp Supply Voltage
2 | BK | 250 | Ground | 2 | BK | 250 | Ground