For 1990-2009 cars

Checks | Actions
--- | ---
Inspect for a worn release bearing. | Replace the worn release bearing.
Inspect for an improperly installed release lever. | Remove and properly reinstall the fork shaft. Very lightly lubricate the fork fingers at the release bearing with wheel bearing grease.
Improper clutch cable adjustment | Adjust clutch cable. Refer to Clutch Assembly Adjustment .
Worn clutch cable | Replace clutch cable. Refer to Clutch Cable Replacement .