For 1990-2009 cars

### Removal Procedure

1. Fold down the rear seat back.
2. Remove the C-pillar trim.
3. Remove the rear seat belt lower anchor bolts. Refer to Shoulder Belt Replacement - Rear .
4. Remove the center high mounted stop lamp. Refer to High Mount Stop Lamp Inoperative .
5. Remove the child seat anchors. Refer to Child Restraint Tether Anchor Replacement .
6. Remove the back panel upper cover.
7. Remove the plastic retaining clips.
8. Slide the deck lid sill plate cover forward to remove.

### Installation Procedure

1. Install the rear deck lid sill plate cover with the plastic retaining clips.
2. Install the back panel upper cover.
3. Install the child seat anchors. Refer to Child Restraint Tether Anchor Replacement .
4. Install the center high mounted stop lamp. Refer to High Mount Stop Lamp Inoperative .
5. Install the rear seat belt lower anchor bolts. Refer to Shoulder Belt Replacement - Rear
6. Install the C-pillar trim panel.
7. Put back the rear seat back.