For 1990-2009 cars

Caution: Refer to Battery Disconnect Caution in the Preface section.

Notice: Any time service is being performed which requires removal of the air cleaner assembly, always cover the throttle body opening. This will prevent any foreign material from entering the engine.

An automobile engine is a combination of many machined, honed, polished, and lapped surfaces with tolerances that are measured in the ten-thousandths of an inch. When any internal engine parts are serviced, care and cleanliness are important. A liberal coating of engine oil should be applied to friction areas during assembly to protect and lubricate the surfaces on initial operation. Proper cleaning and protection of machined surfaces and friction areas is part of the repair procedure. This is considered standard shop practice even if not specifically stated.

Whenever valve train components are removed for service, they should be kept in order. They should be installed in the same locations, and with the same mating surfaces, as when they were removed.