For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the bolts (1) from the frame brace (2).
3. Remove the frame brace (2) from the vehicle.

### Installation Procedure

1. Install the frame brace (2) from the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolts (1) to the frame brace (2) and tighten to 100 N·m (74 lb ft).
3. Lower the vehicle.