For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Adjuster Plug | 12 N·m | 106 lb in
Adjuster Plug Locknut (Tighten) | 70 N·m | 52 lb ft
Adjuster Plug Locknut (Loosen) | 10 N·m | 88 lb in
Air Cleaner Housing Bolts | 12 N·m | 106 lb in
Alternator Adjusting Bolts | 20 N·m | 15 lb ft
Ball Joint Hex Nut | 45 N·m | 33 lb ft
Crossmember to Underbody Nut | 150 N·m | 111 lb ft
Outer Tie Rod Nuts | 54 N·m | 40 lb ft
Outer Tie Rod Hex Nut | 45 N·m | 33 lb ft
Pinion Locknut | 30 N·m | 22 lb ft
Pinion Preload | 0.9-1.7 N·m | 8-15 lb in
Power Steering Fluid Reservoir Attaching Bolts | 7 N·m | 62 lb in
Power Steering Line Fittings-Cylinder End | 28 N·m | 21 lb ft
Power Steering Line Fittings-Valve End | 18 N·m | 13 lb ft
Power Steering Pump Pressure Line Union Nut | 28 N·m | 21 lb ft
Power Steering Pump Pulley Bolts | 25 N·m | 18 lb ft
Power Steering Pump Retaining Bolts | 25 N·m | 18 lb ft
Stabilizer Shaft to Knuckle Bolts | 45 N·m | 33 lb ft
Steering Gear Inlet and Outlet Fitting Nuts | 28 N·m | 21 lb ft
Steering Gear Inlet Pipe Fittings | 28 N·m | 21 lb ft
Steering Gear Outlet Pipe Fittings | 22 N·m | 16 lb ft
Steering Gear Retaining Bracket Nuts | 50 N·m | 37 lb ft
Steering Gear Yoke Plug | 5 N·m - 45° | 44 lb in - 45°
Steering Gear Yoke Plug Lock Nut | 44 N·m | 32 lb ft
Tie Rod | 100 N·m | 75 lb ft