For 1990-2009 cars

### Removal Procedure

1. Open the hatchback door.
2. Remove the luggage compartment rear trim panel. Refer to Rear Compartment Trim Panel Replacement .
3. Remove the screws that secure the lock striker.
4. Disconnect the cable from the lock striker.

### Installation Procedure

1. Connect the cable to the lock striker.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the lock striker with the screws.

Tighten
Tighten the hatchback door lock striker screws to 20 N·m (15 lb ft).

3. Install the luggage compartment rear trim panel. Refer to Rear Compartment Trim Panel Replacement .
4. Close the hatchback door.