For 1990-2009 cars

### Removal Procedure

Caution: Refer to Fuel Vapors in Evaporative Emission Components Caution in the Preface section.

1. Disconnect the evaporative emission (EVAP) canister fuel vapor hoses.
2. Remove the bolt securing the EVAP canister flange to the vehicle.
3. Slide the EVAP canister out of the track holder.
4. Remove the EVAP canister.

### Installation Procedure

1. Insert the EVAP canister into the track and slide it into position.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the EVAP canister flange bolt.

Tighten
Tighten the EVAP canister flange bolt to 20 N·m (15 lb ft).

3. Connect the canister fuel vapor hoses.