For 1990-2009 cars

## Child Restraint Tether Anchor Replacement Five Door

### Removal Procedure

1. Open the tether anchor access cap.
2. Remove the bolt and the tether anchor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the tether anchor with the bolt.

Tighten
Tighten the child seat tether anchor bolt to 25 N·m (18 lb ft).

2. Close the tether anchor access cap.

## Child Restraint Tether Anchor Replacement Four Door North America

### Removal Procedure

1. Open the tether anchor cover.
2. Remove the bolt (1) and the tether anchor (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the tether anchor (2) with the bolt (1).

Tighten
Tighten the child seat tether anchor bolt to 38 N·m (28 lb ft).

2. Close the tether anchor cover.

## Child Restraint Tether Anchor Replacement Four Door Except North America

### Removal Procedure

1. Open the tether anchor access cap.
2. Remove the bolt and the tether anchor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the tether anchor with the bolt.

Tighten
Tighten the child seat tether anchor bolt to 25 N·m (18 lb ft).

2. Close the tether anchor access cap.