For 1990-2009 cars

## Fascia Grille Replacement Notchback

### Removal Procedure

1. Open the hood.
2. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
3. Remove the screws and the radiator grille.

### Installation Procedure

1. Install the radiator grille with the screws.
2. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .
3. Close the hood.

## Fascia Grille Replacement Hatchback

### Removal Procedure

1. Open the hood.
2. Remove the screws and the radiator grille.

### Installation Procedure

1. Install the radiator grille with the screw.
2. Close the hood.