For 1990-2009 cars

### Removal Procedure

Notice: Refer to Fuel Pressure Notice in the Preface section.

1. Relieve the fuel system pressure. Refer to Fuel Pressure Relief .

Caution: Refer to Battery Disconnect Caution in the Preface section.

2. Disconnect the negative battery cable.
3. Disconnect the inlet/outlet fuel lines by moving the line connector lock forward and pulling the hose off of the fuel filter tube.
4. Disconnect the fuel filter ground.
5. Remove the fuel filter bracket bolts.
6. Pull the fuel filter out of the retaining clamp.

### Installation Procedure

1. Install the new fuel filter into the retaining clamp. Note the flow direction.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the fuel filter bracket bolts.

Tighten
Tighten the fuel filter bracket bolts to 4 N·m (35 lb ft.

3. Connect the inlet/outlet lines. Secure the lines with the connector lock.
4. Connect the negative battery cable.
5. Perform a leak test of the fuel filter.