For 1990-2009 cars

## Instrument Panel Center Trim Panel Replacement Hatchback

### Removal Procedure

1. Remove the instrument panel center lower cover. Refer to Instrument Panel Lower Trim Panel Replacement .
2. Remove the screws and the instrument panel center upper cover.
3. Disconnect the electrical connector.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Instal the instrument panel center upper cover.

Tighten
Tighten the instrument panel center upper cover screws to 4 N·m (35 lb in).

2. Install the instrument panel center lower cover. Refer to Instrument Panel Lower Trim Panel Replacement .