For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Pry off the interior courtesy lamp lens.
3. Remove the screws and the lamp/power sunroof control switch.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the lamp/power sunroof control switch with the screws.

Tighten
Tighten the interior courtesy lamp/power sunroof control switch screws to 4 N·m (35 lb in).

3. Install the interior courtesy lamp lens.
4. Connect the negative battery cable.