For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the left and the right rear rocker trim panels.

Refer to Rear Side Door Sill Plate Replacement .

3. Remove the rear seat back. Refer to Rear Seat Back Replacement .
4. Remove the bolts and the left and the right lower front seat belt anchors from the lower/center pillar.
5. Remove the left and the right lower B-pillar trim panels. Refer to Rear Side Door Sill Plate Replacement .
6. Remove the front seats. Refer to Front Seat Replacement - Bucket in Seats.
7. Pry off the left and the right front rocker trim panels.
8. Remove the floor console. Refer to Front Floor Console Replacement in Instrument Panel , Gages and Console.

9. Remove the floor carpet.

### Installation Procedure

1. Install the floor carpet.
2. Install the floor console. Refer to Front Floor Console Replacement in Instrument Panel , Gages and Console.
3. Install the left and the right front rocker, trim panels.
4. Install the front seats. Refer to Front Seat Replacement - Bucket in Seats.

5. Install the left and the right lower B-pillar trim panels. Refer to Center Pillar Lower Trim Panel Replacement .

Notice: Refer to Fastener Notice in the Preface section.

6. Install the left and the right lower front seat belt anchors to the lower/center pillar with the bolts.

Tighten
Tighten the seat belt anchor bolts to 35 N·m (26 lb ft).

7. Install the rear seatback. Refer to Rear Seat Back Replacement .

8. Install the left and the right rear rocker trim panels. Refer to Rear Side Door Sill Plate Replacement .

9. Connect the negative battery cable.