For 1990-2009 cars

### Removal Procedure

1. Open the luggage compartment.
2. Remove the luggage compartment rear trim panel. Refer to Rear Compartment Trim Panel Replacement.
3. Remove the bolts that secure the lock striker.
4. Pull the lock striker out.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the lock striker with the bolts and tighten to 8 N·m (71 lb in).
2. Instal the luggage compartment rear trim panel. Refer to Rear Compartment Trim Panel Replacement.