For 1990-2009 cars

### Removal Procedure

1. Remove the bolts that secure the rear portion of the seat to the floor.
2. Remove the bolts that secure the front portion of the front seat to the floor.
3. Disconnect the electrical connector from the driver seat.
4. Remove the seat.

### Installation Procedure

1. Connect the electrical connector to the driver seat.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts into the front and rear portion of the front seat.

Tighten
Tighten the front and rear bucket seat bolts to 25 N·m (18 lb ft).