For 1990-2009 cars

Table 1: | Clock
Table 2: | Ignition Key Alarm Switch
Table 3: | Instrument Cluster
Table 4: | Multifunction Alarm Module
Table 5: | Oil Pressure Switch

#### Clock

Connector Part Information |

• | KM 01-20DS-HU

• | 20-Way M (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | - | - | Not Used
2 | RD | 122 | Rear Fog Lamp Supply Voltage (Rear Fog Lamps)
RD/WH | 740
3 | D-GN/WH | 157 | Courtesy Lamp Control
4 | L-GN | 867 | ABS Warning Indicator Control (w/ABS)
5 | OG | 540 | Battery Positive Voltage
6 | BK | 450 | Ground
7 | D-GN/YE | 358 | Air Bag Indicator Control (w/Tach) LHD
WH | Air Bag Indicator Control (w/Tach) RHD
8 | L-BU | 318 | Front Fog Lamp Supply Voltage (w/Front Fog Lamps)
WH/YE | 1769
9 | BK/WH | 238 | Seat Belt Switch - Driver (w/Tach)
10 | YE | 749 | Security Indicator Control
11 | BN/BK | 419 | Malfunction Indicator Lamp (MIL) Control (w/Tach)
12 | -- | -- | Not Used
13 | D-GN | 31 | Oil Pressure Indicator Control (w/Tach)
14 | YE | 1481 | Hold Mode Indicator Control
15 | YE | 43 | Accessory Voltage
16 | BN/WH | 309 | Right Park Lamp Supply Voltage
17 | PK | 239 | Ignition 1 Voltage
18 | PU | 1358 | Passenger Air Bag Off Indicator Control
19 | D-BU | 25 | Charge Indicator Control/Charge Indicator Signal (w/Tach)
20 | YE | 18 | Hazard Indicator Control

#### Ignition Key Alarm Switch

Connector Part Information |

• | KET MG 610070

• | 2-Way F 090 (2.3 mm) Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 340 | Battery Positive Voltage
2 | L-GN | 80 | Key In Ignition Switch Signal

#### Instrument Cluster

Connector Part Information |

• | KET MG 611336

• | 26-Way F PCB Connector (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH | 30 | Fuel Level Sensor Signal
2 | D-GN/WH | 817 | Vehicle Speed Signal
3 | WH | 121 | Engine Speed Signal
4 | WH | 135 | Engine Coolant Temperature (ECT) Sensor Gauge Signal
5 | PU | 172 | Low Fuel Indicator Control
6 | BN | 33 | Brake Warning Indicator Control
BN/WH
7 | WH | 15 | Right Turn Signal Lamps Supply Voltage
8 | GY/D-GN | 11 | Headlamp High Beam Supply Voltage (Except North America)
L-GN | Headlamp High Beam Supply Voltage (North America)
9 | D-BU | 14 | Left Turn Signal Lamps Supply Voltage
10 | OG | 640 | Battery Positive Voltage
11 | PK | 239 | Ignition 1 Voltage
12 | BN/WH | 309 | Right Park Lamp Supply Voltage
13 | BK | 450 | Ground (w/o Dimming)
L-GN/RD | 230 | Instrument Panel Lamps Dimming Control (w/Dimming)
14 | BK | 450 | Ground
15-16 | -- | -- | Not Used
17 | D-BU | 25 | Charge Indicator Control/Charge Indicator Signal (w/o Tach)
18 | BN/BK | 419 | Malfunction Indicator Lamp (MIL) Control (w/o Tach)
19 | D-GN | 31 | Oil Pressure Indicator Control (w/o Tach)
20 | BK/WH | 238 | Seat Belt Switch - Driver (w/o Tach)
21 | WH | 629 | Daytime Running Lamp (DRL) On Indicator Control (w/o Tach)
22 | RD | 122 | Rear Fog Lamp Supply Voltage (w/o Tach)
23 | D-GN/WH | 358 | Air Bag Indicator Control (w/o Tach)
24 | OG | 640 | Battery Positive Voltage (w/o Tach)
25 | D-GN/WH | 157 | Courtesy Lamp Control (w/o Tach)
26 | BK | 450 | Ground

#### Multifunction Alarm Module

Connector Part Information |

• | KET MG 610896

• | 8-Way F PCB Connector SDL-II PCB Hsg (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK/WH | 238 | Seat Belt Switch - Driver
2 | L-GN | 80 | Key In Ignition Switch Signal
3 | PU/WH | 821 | Engine Overspeed Indicator Control
4 | PU | 126 | Left Front Door Open Switch Signal
5 | BK | 450 | Ground
6 | BN/WH | 309 | Right Park Lamp Supply Voltage
7 | -- | -- | Not Used
8 | PK | 239 | Ignition 1 Voltage

#### Oil Pressure Switch

Connector Part Information |

• | AK 32104

• | 1-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN/WH | 31 | Oil Pressure Indicator Control