For 1990-2009 cars

### Removal Procedure

1. Remove the crossmember assembly. Refer to Front Suspension Crossmember Replacement .
2. Remove the stabilizer bar from the crossmember assembly by removing the U-clamp bolts.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the U-clamps and the stabilizer bar to the crossmember.

Tighten
Tighten the U-clamp bolts to the crossmember assembly to 25 N·m (18 lb ft).

2. Install the crossmember assembly. Refer to Front Suspension Crossmember Replacement .