For 1990-2009 cars

## Blower Motor Relay Replacement Hatchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel fuse cover.
3. Pull out the relay at the front of the relay box.

### Installation Procedure

1. Align the relay contacts with the relay terminal slots.
2. Push the relay firmly into the base. The relay must be seated and flushed with the base edge.
3. Replace the instrument panel access panel.
4. Replace the remote mirror/lighting control panel.
5. Connect the negative battery cable.