For 1990-2009 cars

### Disassemble Procedure

#### Special Tools

• | EN-49074 Universal Valve Spring Compressor

• | EN-49155 Valve Spring Compressing Adapter

• | KM-845 Suction Device

Note: Take extreme care to prevent any scratches, nicks or damage to the camshaft surfaces.

1. Remove the camshaft position solenoid valve housing.
2. Remove the camshaft cap bolts in this sequence (1)-(4)-(2)-(3).
3. Remove the camshaft caps.
4. Remove the camshafts (1, 2) and oil seal rings (3).
5. Remove the valve tappet using the KM-845 suction device .
6. Install the EN-49074 compressor and EN-49155 adapter .
7. Remove the valve key.
8. Remove the valves (5), springs (3), retainers (2), and seals (4).