For 1990-2009 cars

### Removal Procedure

1. Remove the door seal trim. Refer to Door Water Deflector Replacement .
2. Remove the screw securing the door handle to the door.
3. Disconnect the inside door handle and the lock rods.

### Installation Procedure

1. Connect the inside door handle and the lock rods.
2. Insert the inside door handle into the slots in the door.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the inside door handle screw.

Tighten
Tighten the inside door handle screw to 3 N·m (27 lb in).

4. Install the door seal trim. Refer to Door Water Deflector Replacement .