For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear window wiper arm. Refer to Rear Window Wiper Arm Replacement.
3. Remove the hatchback door lower garnish molding.
4. Remove the bolts and the rear wiper motor.
5. Disconnect the electrical connector.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Connect the electrical connector.
2. Install the rear wiper motor with the bolts.

Tighten
Tighten the wiper motor bolts to 9 N·m (80 lb in).

3. Install the hatchback door lower garnish molding.
4. Install the rear window wiper arm. Refer to Rear Window Wiper Arm Replacement.
5. Connect the negative battery cable.