For 1990-2009 cars

### Removal Procedure

1. Disconnect the hood release cable from the hood latch release handle.
2. Remove the I/P undercover.
3. Remove the driver side knee bolster.
4. Disconnect the tire pressure module connector.
5. Remove the tire pressure module retaining screws and the module (1).

### Installation Procedure

1. Install the tire pressure module (1). Secure with retaining screws.
2. Connect the tire pressure module connector.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the driver side knee bolster and tighten to 10 N·m (89 lb in).
4. Install the I/P undercover.
5. Connect the hood release cable to the hood latch release handle.