For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Coolant Pump Mounting Bolts | 10 N·m | 89 lb in
Electric Cooling Fan Assembly Mounting Bolts | 4 N·m | 35 lb in
Electric Cooling Fan Motor Nut | 3.2 N·m | 28 lb in
Electric Cooling Fan Motor Retaining Screws | 4 N·m | 35 lb in
Negative Battery Terminal Retainer Bolt | 15 N·m | 11 lb ft
Surge Tank Attaching Bolt | 10 N·m | 89 lb in
Thermostat Housing Mounting Bolts | 20 N·m | 15 lb ft
Upper Left Radiator Retaining Bolt | 7 N·m | 62 lb in
Upper Right Radiator Retaining Bolt | 7 N·m | 62 lb in