For 1990-2009 cars

## Radio Antenna Module Replacement Notchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement.
3. Disconnect the negative battery cable.
4. Remove the screws and the glass antenna module.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the glass antenna module with the screws and tighten to 2.5-3.5 N·m (22-31 lb in).
2. Connect the electrical connectors.
3. Install the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement.
4. Connect the negative battery cable.

## Radio Antenna Module Replacement Hatchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the interior courtesy lamp. Refer to Interior Courtesy Lamp Replacement.
3. Remove the screw from the vehicle inside.
4. Remove the roof antenna.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the roof antenna with the screw and tighten to 3 N·m (27 lb in).
2. Install the interior courtesy lamp. Refer to Interior Courtesy Lamp Replacement.
3. Connect the negative battery cable.