For 1990-2009 cars

### Removal Procedure

1. Remove the fuel pump. Refer to Fuel Pump Replacement.
2. Disconnect the insulator connector.
3. Push the terminal wedge (1) in the insulator connector.
4. Push the wedge (1) outside and then pull the wires to disconnect from the insulator.
5. Remove the fuel level sensor (1) from the sender housing (2).
6. Remove the fuel sender assembly (1).

### Installation Procedure

1. Wind the wires (1) to the sender assembly (2)..
2. Install the sender assembly onto the fuel pump assembly (1).
3. Install the fuel level sensor onto the sender housing.
4. Connect the wire into the insulator connector.
5. Connect the insulator connector.
6. Install the fuel pump. Refer to Fuel Pump Replacement.